# MCXFLASHNT documentation rev. A 2003/09/01

## MCXFLASHNT - Flash memory update program for the MCXPCI

English text (Version française)

MCXFLASHNT.EXE is located in the "driver" directory.

In order to use MCXFLASHNT.EXE you must take the following steps:

- Check that SW1-1 and SW1-2 are both set to OFF (Built-in firmware mode, this is the factory setting)
- Install the MCXPCI card in the PC
- Install the MCXNT driver (version 2.1.4 or greater)
- With MCXSETUP, select the "MCXDOS/AUTOMCX" mode for the card (yes, this contradicts the switch settings)
- With MCXSETUP, check the device name that was given to the card (i.e. "COM")
- Have the MCXFLASHNT executable and the flash image file ("mLITE570.FLH" for example) in the same directory
- Start a command prompt window, go to that directory, and type a command similar to:

      mcxflashnt devicename FlashImageFile
      for example :
      mcxflashnt com mLITE570.FLH

- If needed, switch back the SW1-1 and SW1-2 switches
- If needed, set back the mode of the card in MCXSETUP.

## MCXFLASHNT - Programme de mise à jour de mémoire flash pour MCXPCI

Texte français (English version)

Vous pouvez trouver MCXFLASHNT.EXE dans le répertoire "driver".

Pour utiliser MCXFLASHNT.EXE conformez-vous aux instructions suivantes:

- Vérifiez que SW1-1 et SW1-2 sont tous deux en position OFF (mode Built-in firmware, c'est la configuration usine)
- Installez la carte MCXPCI dans le PC
- Installez le pilote MCXNT (version 2.1.4 ou supérieure)
- Avec MCXSETUP, choisissez le mode "MCXDOS/AUTOMCX" pour la carte (ceci contredit la position des switchs, c'est normal)
- Avec MCXSETUP, informez-vous du nom de périphérique qui a été assigné à la carte (en général "COM")
- Placez l'exécutable MCXFLASHNT et le fichier image flash ("mLITE570.FLH" par exemple) dans le même répertoire
- Lancez une fenêtre invite de commande, allez dans ce répertoire, et tapez une commande du type:

      mcxflashnt devicename FlashImageFile
      par exemple :
      mcxflashnt com mLITE570.FLH

- Si nécessaire, replacez les interrupteurs SW1-1 et SW1-2 dans leur position d'origine
- Si nécessaire, remettez le mode de fonctionnement correct pour la carte dans MCXSETUP.