# ACKSYS WaveOS

Changes Log Known issues

## Version 3.18.1.1 release notes

### Documentation

- A User's guide referenced DTUS070 provides information common to all products supported by WaveOS.
- Installation guides provide data specific to each product. They are written both in English and French.
- The Acksys NDM software helps configure and monitor Acksys's Wi-Fi products. It installs in English or French, and comes with online help in English.

Documentation and Acksys NDM are available from the CDROM or from the Acksys website (www.acksys.com).

### Downgrading to version 2.x.x.x on WLn range

If you absolutely need to downgrade to 2.x.x.x release, after the download-and-reboot process is finished, you must reset it to factory settings before reconfiguring it and using it again.
So it may be unadviseable to do a downgrade on the field.

### Upgrading from version 2.x.x.x on WLn series

If you upgrade a product of the WLn series from version 2.x.x.x to version 3.8.0.1 or older, the first byte of WiFi MAC address can change. If your architecture include repeaters, or MAC address filtering, configuration changes may be necessary on the concerned devices.

## Changes Log

Version / date | Changes
--- | ---
3.18.1.1 19-November-2018 | Bug fixes and improvement
Improve the wifi enable/disable management in the web interface Fix issues:#2574,#2575,#2581
3.18.0.1 17-October-2018 | Bug fixes and improvement
Add event-driven IP interface selection. That allows switching route between LTE, WiFi, Ethernet. SRCC: Allow the pre-shared key configuration Add AirXroad support Add RuggedAir range support Allow firmware upgrade for LTE card Allow to use a non RSA private Key Fix issues:#2448, #2464, #2466., #2470, #2501., #2503, #2532., #2544, #2560., #2561, #2562.
3.16.1.1 3-July-2018 | Bug Fixes and improvement
Add GNSS/LTE status in SNMP Support Acksys MIB 3.10.6.1 Add GNSS status Add LTE status Fix issues: #2425,#2446
3.16.0.1 25-April-2018 | Improvement
Add AirBox support Add GNSS and LTE support.
3.14.5.1 30-August-2018 | Bug fixes
Fix issues:#2472, #2474, #2486, #2488.
3.14.3.1 02-July-2018 | Bug fixes and improvement
Fix issues:#2423, #2427, #2428, #2443, #2444. In roaming settings, force client disconnection on duration for min/max threshold
3.14.2.1 15-May-2018 | Bug fixes
Fix issues:#2409, #2413, #2416, #2417
3.14.1.1 18-April-2018 | Bug fixes
Fix issues:#2359, #2369, #2371, #2379, #2389, #2390, #2391, #2399, #2403
3.14.0.1 7-March-2018 | Improvements and bug fixes
Add "user" login account to show the product status. This login can't change/show the product settings. Add openVPN support (client and server) Update the Quatar regulatory domain Add parameter to allow the wifi client to send a deauthentication frame to the AP leaved

- Fix Key Reinstallation Attacks (KRACK)
- Support ACKSYS-MIB version 3.10.4.1
  - Add SAE (Mesh security) support
  - Add product identification support
- Fix issues: #878,#1696,#1955, #2058,#2234,#2318,#2343
3.12.14.1
5-February-2018 bug fix

- Fix issue: #2319

3.12.13.1
5-February-2018 bugs fixes

- Fix issues: #2311, #2321

3.12.12.1
24-november-2017 Improvement and bugs fixes

- Fix issues: #2250, #2254, #2255, #2273, #2275
- Add config status web page, to check the configuration.
- Add SRCC deamon status web page

3.12.11.1
16-october-2017 Improvement and bug fixes

- Fix issues: #2156, #2161 #2218, #2226 #2235
- Add hostname option in DHCP settings
- Add DHCP information in status/network web page
- Add DNS server information in status/network web page

3.12.10.1
21-september-2017 Improvements and bug fixes

- Support ACKSYS-MIB version 3.10.3.1
- Add srcc link status
- Fix issues: #2212, #2220 #2209, #2210

3.12.9.1
30-august-2017 Improvements and bug fixes

- Support ACKSYS-MIB version 3.10.2.1
  - Add Mesh survey table
  - Add Input filter groups settings
  - Add somes Wireless advanced settings
  - Add SRCC settings
- Add input bridge filter
- Fix issues: #2164, #2165, #2182, #2183, #2189

3.12.8.1
12-july-2017 Improvements and bug fixes

- Upgrade Pim deamon. That fix some issues and improve the protocol performance.
  → WARNING: This upgrade is not compatible with the previous version. You must upgrade all products.
- Fix VRRP protocol management. That fix some issues (static route not applied, GRE tunnel not enable when VRRP is master, ...).
  → WARNING: With this fix it is not possible to have VRRP and DHCP protocol on the same network.
- Add persistence parameter in the advanced network settings.
- fix issues:#2095,#2141,#2144,#2150,#2151,#2154

3.12.7.1
16-june-2017 Improvements and Bug Fixes

- Reduction of packet loss on highest WMM QOS in case of network congestion: #2063
- Add EmbedAir 1000 products range support
- Add onlink parameter in static routes settings
- Fix issues: #2116,#2097

3.12.6.1
30-may-2017 Improvements and Bug Fixes

- Roaming improvements: #2061,#2096,#2112
- Enable routing in L25NAT mode with local router: #2098
- Fix issues: #2109

3.12.5.1
22-may-2017 Improvement

Support of WaveManager Version 1.0.0.0

3.12.4.1
11-may-2017 Bug Fixes

- Fix issues: #2086,#2087

3.12.3.1
04-may-2017 Improvements and Bug Fixes

- Support ACKSYS-MIB version 3.10.0.1

- Add some OID for network status
- Add an OID to return the hash result of the configuration
- Add OID to allow a binary file transfert to the product

- Update remote access security for advanced users
- Fix issues: #2049,#2051, #2056,#2057,

3.12.2.1
13-april-2017 Improvements and Bug Fixes

- Configuration of buffer size for power saving stations in the AP
- Fix issues: #2012,#2023, #2031,#2036, #2042,#2044, #2045,#2046, #2047,

3.12.0.1
16-march-2017 Improvements and Bug Fixes

- Management of VLAN priority on 802.1Q VLAN interfaces
- Set localhost and ip destination to firewall rules
- Adding source ip field to firewall rules
- Adding frame protocol GRE to firewall rules
- Adding sort of the firewall rules
- VRPP: Add unicast peer for Advertisement
- VRRP: Add multicast group settings
- Add EmbedAir range products support
- Support Acksys MIB version 3.8.8.1

- Add WiFi association table
- Add wired ethernet interface status

- Add DFS channel support on mesh mode
- Management of GRE endpoints on VRRP virtual addresses
- Fixing VRRP virtual IP loss by virtual VLAN interfaces after link down then link up
- Deleting GRE static route from configuration after Gre interface deletion from config file
- Fix issues: #1629, #1948,#1963, #1992,#1996, #1951, #2005,#2007,

3.10.2.1
31-jan-2017 Bug Fixes

- Fix issue #1946

3.10.1.1
16-jan-2017 Bug Fixes

- Management of VLAN interfaces on Wifi interfaces with Client STA roles
- Fix issue #1910
- Fix issue #1911

3.10.0.1
13-dec-2016 Bug Fixes and MIB improvement

- Support ACKSYS-MIB version 3.8.6.1

- Add 802.11ac settings
- Add Wifi multichannel management
- Add GRE settings
- Add Roaming settings
- Add network friendly name
- Add gateway in network settings
- Allow to set a bridge on network settings
- Allow to show the WPA preshared key with SNMP V3 in default settings
- Improvement WPA security management
- Bug Fixes on somes OID
- Fix IP format error in somes OID

- Improve the status Association list in product web page
- Improve the SRCC log message
- Update SSL library to fix some security issue
- Fix issue #1727,#1826,#1841,#1846, #1856,#1863,#1875,#1887

3.8.0.1
14-oct-2016 Bug Fixes and Wln range support

- Add WLn range support
- Support ACKSYS-MIB version 3.8.5.1

- Add OID to download the WPA user certificat
- Add OID to configure the DNS relay
- Add OID to set the WPA key life time
- Add OID to set the off-channel delay for the active scan in roaming mode
- Add OID to know the RSTP status

- Add Discover agent password setting
- Clonning: Add Pre-connect feature
- Add support HT40 automatic for client mode
- Fix issue #1432,#1553,#1719,#1721, #1768,#1774,#1787

3.6.0.1
23-July-2016 Bug Fixes and improvement

- Add PIMd support
- SRCC: Allow tx power settings
- SRCC: Send log to product syslog
- Add static clonning support
- Add IP alias settint
- Add bandwith tools in Web interface
- Add spectral analyzer for 11n card
- Add graphical view of WiFi scan
- Add wifi service status
- Add SNMP V3 OID to enable/disable ssh server
- Fix issue #1591,#1663,#1677,#1685

3.4.2.1
12-april-16 Bug Fixes and improvement

- Fix issue #1637 : If the password file is corrupted, the upgrade will close the web access for security reason. You must restore the factory settings and restore your settings.
- Add RSTP daemon monitoring.

3.4.1.1
22-march-16RSTP improvement

- Improve the RSTP link down detection on the wireless interface when she is overload.

3.4.0.1
09-march-16Bug fixes and Firmware improvements

- Add VRRP support.
- Add SRCC mixed redundant mode: Add redundant coupling topology with 1 wired link and WiFi link.
- MCS list configuration: On RailBox/11, allow to set the MCS list supported by the AP.
- Add SNMP V3 support
- Managed settings compatibility with WLn series
- Add bandwith graphics in Web Interface
- Fix issues #1481,#1506,#1537,#1543,#1555 ,#1562,#1568

3.2.0.1
27-november-15First WaveOS release

- QOS support : QOS supports up to 7 priority levels. Shares the availabe priority level bandwidth between all streams.
- SRCC support : Automatic solution for the carriage coupling.
- RSTP support: Rapid Spaming Tree allows ring network topoligy and redundant network.
- L2 GRE tunnel support
- Support VLAN in the bridge
- Disable WiFi service if network host does not respond to the ping
- Send trap when DFS event occurs

back to top

## ACKSYS WaveOS known issues

Please note that several problems reported to our technical support were found as customer problems or non-bugs, thus the holes in the numbered list below.
When provided, countermeasures apply until the issue is closed.

Tracker# | found in versions | version corrected | Description / Countermesures
--- | --- | --- | ---
878 | 3.0.0.1 | 3.14.0.1 | The OID statusPhyWifiScanTableUpdateTbl may return 'Available' when the scan is finished. →Update to 3.14.0.1
1432 | 3.2.0.1 | 3.8.0.1 | With some web browser, it can be impossible to commit the wireless settings. →Update to 3.8.0.1
1480 | 3.2.0.1 |  | It is not possible to send VLAN tagged frames through the WiFi interface. →use L2 GRE tunnel on wireless interface if you need to send VLAN tagged frames.
1481 | 3.2.0.1 | 3.4.0.1 | On RailBox/11, the connection between the AP and the sta can be dropped during the WPA rekeying. →Set the rekeying delay to 0.
1506 | 3.2.0.1 | 3.4.0.1 | On RailBox/11, the SAE security doesn't work. →Upgrade to 3.4.0.1
1537 | 3.2.0.1 | 3.4.0.1 | The frame filter on GRE interface doesn't work.
1543 | 3.2.0.1 | 3.4.0.1 | The wireless clonning mode doesn't work
1553 | 3.2.0.1 | 3.8.0.1 | In some cases, it is possible to have an incomplete GRE tunnel configured, and it is not possible to delete it.
1555 | 3.2.0.1 | 3.4.0.1 | If the bridge VLAN feature is enabled on the bridge and a wireless interface is added in the bridge and the wireless interface uses the automatic channel select or DFS channel, the bridge VLAN settings are not applied.
1562 | 3.2.0.1 | 3.4.0.1 | The administrator password is not exported in the C-KEY nor the configuration file.
1568 | 3.2.0.1 | 3.4.0.1 | The wireless "g only" mode is not compatible between the WLg and Railbox series. →Use the "b/g" mode instead.
1591 | 3.4.0.1 | 3.6.0.1 | Access to the web interface with HTTPS protocol doesn't work. →Upgrade to 3.6.0.1
1629 | 2.8.0.1 | 3.12.0.1 | The scan result get from snmp, the latest mac address byte is missing. →Upgrade to 3.12.0.1
1637 | 3.4.0.1 | 3.4.2.1 | If the password file is corrupted, the web interface access is not protected. The password can be corrupted if you change the password and power off the product, while the modifications are saved. →Upgrade to 3.4.2.1
1663 | 3.0.0.1 | 3.6.0.1 | The https server is vulnerable to several SSL attack (Hearthbleed, CCS injection, Poodle, ...). →Upgrade to 3.6.0.1
1677 | 3.0.0.1 | 3.6.0.1 | The settings backup file list are not the same between the C-Key and the web interface backup. →Upgrade to 3.6.0.1
1685 | 3.4.2.1 | 3.6.0.1 | the "Wireless/channel status" web page is not available. →Upgrade to 3.6.0.1
1696 | 3.5.0.1 | 3.14.0.1 | The OID internalAlarmSwitch doesn't return the Switch status →Upgrade to 3.14.0.1
1719 | 3.6.0.1 | 3.8.0.1 | In some cases, it is possible to have an internal error on Vlan bridge settings. →Upgrade to 3.8.0.1
1721 | 3.4.0.1 | 3.8.0.1 | Wireless mesh mode is not compatible with DFS. Add check in the wireless settings →Upgrade to 3.8.0.1
1727 | 3.0.0.1 | 3.10.0.1 | If the GRE local IP is not reachable when the GRE is initialized, all GRE traffic are send to the gateway. →Upgrade to 3.10.0.1
1768 | 3.6.0.1 | 3.8.0.1 | In setup/physical interfaces overview, one error occur if the user select several channels in interface settings. →Upgrade to 3.8.0.1
1774 | 3.6.0.1 | 3.8.0.1 | The MCS list is not generated on RailBox/21 and RailBox/25 →Upgrade to 3.8.0.1
1787 | 3.6.0.1 | 3.8.0.1 | If the user change the product time zone, the product stay in UTC time zone. →Upgrade to 3.8.0.1
1826 | 3.6.0.1 | 3.10.0.1 | In some cases the SRCC association can failed or is slow. →Upgrade to 3.10.0.1
1841 | 3.8.0.1 | 3.10.0.1 | On Wln platform, the graphical bandwidth report doesn't work. →Upgrade to 3.10.0.1
1846 | 3.8.0.1 | 3.10.0.1 | If the 802.11w is enable on the AP, it is doesn't work correctly. →Upgrade to 3.10.0.1
1856 | 3.8.0.1 | 3.10.0.1 | In setup/physique interface page the filters group link doesn't work.
1863 | 3.6.0.1 | 3.10.0.1 | The timezone settings is not correctly applied. →Upgrade to 3.10.0.1
1875 | 3.6.0.1 | 3.10.0.1 | The access to the page status wirless is not possible if all wireless card are disabled
1887 | 3.8.0.1 | 3.10.0.1 | With chrome version 55 some web page are not showed corretly. →Upgrade to 3.10.0.1
1910 | 3.10.0.1 | 3.10.1.1 | The mesh SAE security don't work correctly with another WaveOS version. →Upgrade to 3.10.1.1
1911 | 3.10.0.1 | 3.10.1.1 | It is not possible to create an VLAN Virtual interface on Wifi interface on mesh. →Upgrade to 3.10.1.1
1946 | 3.10.0.1 | 3.10.2.1 | If you use SRCC on wifi 1 and AP on wifi 2, on certainly case the AP on wifi 2 can be disable during the SRCC association. →Upgrade to 3.10.2.1
1948 | 3.11.0.5 | 3.11.0.51 | snmpd: fix engineID management →Upgrade to 3.11.0.51
1951 | 3.10.0.1 | 3.12.0.1 | In the web server, when the site survey is finished, in certainly case we don't see the result but we are redirected to the home page. →Upgrade to 3.12.0.1
1955 | 3.11.0.1 | 3.14.0.1 | It is not possible to change the Radius port in WPA/WPA2 settings. →Upgrade to 3.14.0.1
1963 | 3.11.0.5 | 3.11.0.51 | Fix snmpd agent version v3 value →Upgrade to 3.11.0.51
1992 | 3.10.0.1 | 3.12.0.1 | When the product is upgraded with NDM, the upgrade result from the product is "saving config files". →Upgrade to 3.12.0.1
1996 | 3.10.0.1 | 3.12.0.1 | In certanly case, the product can crash after several VRRP switch over. →Upgrade to 3.12.0.1
2005 | 3.10.0.1 | 3.12.0.1 | When the VRRP logs are enabled, some time the product can crash. →Upgrade to 3.12.0.1
2007 | 3.10.0.1 | 3.12.0.1 | In multicast routing, if the query interval is set to a value higher than 46s, the multicast routing can stop randomly. →Upgrade to 3.12.0.1
2012 | 3.12.0.1 | 3.12.2.1 | Fix system hanging during boot in some rare conditions. →Upgrade to 3.12.2.1
2023 | 3.12.0.1 | 3.12.2.1 | Fix antennas choice list. →Upgrade to 3.12.2.1
2031 | 3.12.0.1 | 3.12.2.1 | Certain advanced mesh parameters are not working properly. →Upgrade to 3.12.2.1
2036 | 3.12.0.1 | 3.12.2.1 | 5GHz channels must not be usable in Israel. →Upgrade to 3.12.2.1
2042 | 3.12.0.1 | 3.12.2.1 | Can not configure bridge broadcast filter per snmp. →Upgrade to 3.12.2.1
2044 | 3.12.0.1 | 3.12.2.1 | Bridge filter is not working. →Upgrade to 3.12.2.1
2045 | 3.12.0.1 | 3.12.2.1 | Bridge filter rules are not applied on ethernet port after a reboot. →Upgrade to 3.12.2.1
2046 | 3.12.0.1 | 3.12.2.1 | Error when displaying traffic class prio status page. →Upgrade to 3.12.2.1
2047 | 3.12.0.1 | 3.12.2.1 | SSIDs of wifi interfaces are not displayed in QOS traffic class prio submenu. →Upgrade to 3.12.2.1
2049 | 3.12.0.1 | 3.12.3.1 | In SRCC, the link establishement can be too long. →Upgrade to 3.12.3.1
2051 | 3.12.0.1 | 3.12.3.1 | In certainly case the discover service response can be not correct. The NDM view can be affected. →Upgrade to 3.12.3.1
2056 | 3.12.0.1 | 3.12.3.1 | If the bridge VLAN feature is enable and all bridge ports don't participate to the sames VLAN, some communication can not work correctly. This bug only affect the RailBox products. →Upgrade to 3.12.3.1
2057 | 3.12.0.1 | 3.12.3.1 | The bridge filter configuration through SNMP, can return some default values. These values are not writen in the configuration file. →Upgrade to 3.12.3.1
2058 | 3.12.0.1 | 3.14.0.1 | Somes OID return the default value even if the value was not set. →Upgrade to 3.14.0.1
2086 | 3.12.3.1 | 3.12.4.1 | In certainly case it is not possible to set the client mode throught the Web interface. The interface return an error during the save process. →Upgrade to 3.12.4.1
2087 | 3.12.3.1 | 3.12.4.1 | A buffer overflow can occure in Acksys Mib library. The result is some no consistant information is returned by the SNMP interface. →Upgrade to 3.12.4.1
2061 | 3.12.4.1 | 3.12.6.1 | Roaming improvement with multiple Vlans topology →Upgrade to 3.12.6.1
2096 | 3.12.4.1 | 3.12.6.1 | Reduction of packet loss during roaming →Upgrade to 3.12.6.1
2098 | 3.12.4.1 | 3.12.6.1 | Enable routing in L25NAT mode with local router →Upgrade to 3.12.6.1
2109 | 3.12.4.1 | 3.12.6.1 | Fix wrong status showed in NDM during roaming →Upgrade to 3.12.6.1
2112 | 3.12.4.1 | 3.12.6.1 | Roaming: Add parameter to control station deauthentication →Upgrade to 3.12.6.1
2063 | 3.12.6.1 | 3.12.7.1 | Reduction of packet loss on highest WMM QOS in case of network congestion →Upgrade to 3.12.7.1
2097 | 3.12.6.1 | 3.12.7.1 | Fix: VRRP stops sending advertisements on an interface after that it has roamed. →Upgrade to 3.12.7.1
2116 | 3.12.6.1 | 3.12.7.1 | VRRP: Fix initialisation issue →Upgrade to 3.12.7.1
2095 | 3.12.2.1 | 3.12.8.1 | Multicast stream doesn't resume after the VRRP master reboot. →Upgrade to 3.12.8.1
2141 | 3.12.5.1 | 3.12.8.1 | The product ID used by NDM/WaveManeger is stored on configuration file and restored during the restore configuration process. If you restore a configuration on a product from another product, NDM, WaveManager will consider the both product as the same product. →Upgrade to 3.12.8.1
2144 | 3.12.7.1 | 3.12.8.1 | Firewall rules without src and dest zone are not displayed in the web interface. →Upgrade to 3.12.8.1
2150 | 3.12.5.1 | 3.12.8.1 | If network loop occure between the product network interface, an kernel crash occurs. →Upgrade to 3.12.8.1
2151 | 3.12.0.1 | 3.12.8.1 | Wifi regulation domain: The chile was changed the regulation rule. Update the regulation domain to respect the new rules. →WARNING: This upgrade will reduce the Txpower to 17dBm on band 5735 - 5835 MHz.
2154 | 3.12.0.1 | 3.12.8.1 | SNMP: Fix some OID to allow router configuration. →Upgrade to 3.12.8.1
2156 | 3.12.0.1 | 3.12.11.1 | SRCC: If the user select a chanel not compatible with the HT40+ mode, SRCC doesn't work →Upgrade to 3.12.11.1
2161 | 3.12.5.1 | 3.12.9.1 | The mono-card repeater doesn't work. →Upgrade to 3.12.9.1
2164 | 3.12.5.1 | 3.12.9.1 | VRRP and static route: If the product have a static route and ip alias, after two VRRP transition (the product back in backup) static route is not correctly set and it is not possible to access at the product from far network. →Upgrade to 3.12.9.1
2165 | 3.12.7.1 | 3.12.9.1 | The roaming log level doesn't show the roaming log. →Upgrade to 3.12.9.1
2182 | 3.10.0.1 | 3.12.9.1 | We can set an IP address with an invalide format wihtout Error in the web page. eg: 192.168.010.20 is invalide because the digit '010' is an octal représentation and it is not supported by the firmware. →Upgrade to 3.12.9.1
2183 | 3.12.0.1 | 3.12.9.1 | In NAT router configuration, some frames can be sent with the ip source set to an private IP. →Upgrade to 3.12.9.1
2189 | 3.12.0.1 | 3.12.9.1 | The bridge filter rules are not correctly applied on Wifi interface in AP mode configured to use a DFS channel. →Upgrade to 3.12.9.1
2209 | 3.12.0.1 | 3.12.1.1 | In snmp statusIfWlanTable, each wlan is present two times. →Upgrade to 3.12.10.1
2210 | 3.10.0.1 | 3.12.10.1 | The association counter (statusIfWlanPeers) don't work in mesh node. →Upgrade to 3.12.10.1
2212 | 3.12.9.1 | 3.12.10.1 | If two vrrp instance are configured in the same network, only one IP is applied. →Upgrade to 3.12.10.1
2218 | 3.12.9.1 | 3.12.11.1 | On EmbedAir and Airlink the WPA and WEP doesn't work. →Upgrade to 3.12.11.1 or use WPA2
2220 | 3.10.0.1 | 3.12.10.1 | In rarely case, the snmp deamon management can generate a configuration corruption. →Upgrade to 3.12.10.1
2226 | 3.12.7.1 | 3.12.11.1 | Fix product hanging in power save mode. →Upgrade to 3.12.11.1
2234 | 3.12.9.1 | 3.14.0.1 | The OID statusIpSubnetMenber from statusIpSubnetTable doesn't not give the list of interface member. →Upgrade to 3.14.0.1
2235 | 3.12.9.1 | 3.12.11.1 | The AP default settings are not the same in SNMP and Web interface →Upgrade to 3.12.11.1 or change the values after the AP is added with the SNMP interface.
2250 | 3.12.11.1 | 3.12.12.1 | The status network web page doesn't work (error 500) if one wifi card is disabled. →Upgrade to 3.12.12.1 or enable all wifi cards on the product.
2254 | 3.12.11.1 | 3.12.12.1 | The multicast routing deamon doens't work correctly when several IP address are set on managed interface. →Upgrade to 3.12.12.1.
2255 | 3.12.11.1 | 3.12.12.1 | The firewall and VRRP configuration files are not well synchronised with network configuration file. →Upgrade to 3.12.12.1.
2273 | 3.10.0.1 | 3.12.12.1 | The wireless status files can be corrupted. →Upgrade to 3.12.12.1 or reset to factory the settings.
2275 | 3.12.11.1 | 3.12.12.1 | The VRRP deamon is not properly stopped when the configuration is reloaded. →Upgrade to 3.12.12.1.
2311 | 3.12.11.1 | 3.12.13.1 | In WiFi client mode, If we received a Deauthentication frame from the AP the client will black list tis AP. In certainly case this list is not purged and the APs is not available for new association. →Upgrade to 3.12.13.1.
2321 | 3.12.11.1 | 3.12.13.1 | The Atheros Adaptive noise imunity doesn't work correctly. This fix can increase the Wifi performance in case of noisy environment. →Upgrade to 3.12.13.1.
2318 | 3.12.12.1 | 3.14.0.1 | The NTP client mays send the request before the interface is ready to forward the data. In this case the time synchronisation will perform on the next update. →Upgrade to 3.14.0.1
2319 | 3.12.12.1 | 3.12.14.1 | In WiFi roaming client mode, a wrong RSSI is sometimes obtained from the Access Points which use a DFS channel. This may result in incorrect selection of the Best AP to roam to. →Upgrade to 3.12.14.1 or, →Reduce the beacon interval on all relevant AP's to less than 70 ms (or 70 TU)
2343 | 3.12.11.1 | 3.14.0.1 | The page status/wireless/assoc in web server may not display →Upgrade to 3.14.0.1.
2359 | 3.14.0.1 | 3.14.1.1 | The web page to show the statistic graph show error and crash on wifi interface. →Upgrade to 3.14.1.1.
2369 | 3.14.0.1 | 3.14.1.1 | On the EmbedAir1000 it is not possible to configure an AP in 802.11ac mode. →Upgrade to 3.14.1.1.
2371 | 3.14.0.1 | 3.14.1.1 | In certainly case the signal level in client scan result is egal to 0. →Upgrade to 3.14.1.1.
2379 | 3.12.10.1 | 3.14.1.1 | In SRCC configuration, if the link is broken, it will be never restablished. →Upgrade to 3.14.1.1.
2389 | 3.14.0.1 | 3.14.1.1 | In system log if the line is too long that can store a line with some garbage. →Upgrade to 3.14.1.1.
2390 | 3.12.13.1 | 3.14.1.1 | If we configure an AP with pre-authentication in some case this feature is not enabled on the AP. →Upgrade to 3.14.1.1.
2391 | 3.14.0.1 | 3.14.1.1 | in mono-channel roaming configuration, the foreground scan doesn't work properly. →Upgrade to 3.14.1.1.
2399 | 3.14.0.1 | 3.14.1.1 | On RaiBox/RailTrack ethernet interface Transmit fifo can overflow and occurs some packet lost. →Upgrade to 3.14.1.1.
2403 | 3.10.0.1 | 3.14.1.1 | In case of the configuration is restored from the C-KEY after an reset to factory settings, the network configuration stay in default settings. →Upgrade to 3.14.1.1.
2409 | 3.12.7.1 | 3.14.2.1 | If the product is set in DHCP mode, in Wifi client mode and bridging mode in ARPNAT, the product will reboot each time it should renew the DHCP lease. →Upgrade to 3.14.2.1 or use the WDS bridging mode (not compatible with roaming).
2413 | 3.14.0.1 | 3.14.2.1 | The status page status/wireless/services_status will generate an error in syslog. →Upgrade to 3.14.2.1.
2416 | 3.14.0.1 | 3.14.2.1 | If the product is set in DHCP mode, in Wifi client mode and bridging mode in ARPNAT, the checksum is wrong in the first renew frame sent. The renew at half lease dont' work properly. →Upgrade to 3.14.2.1.
2417 | 3.14.1.1 | 3.14.2.1 | The factory settingss on RailBox is wrong. The ip address is set to 192.168.1.1 and only LAN1 is in the default bridge. →Upgrade to 3.14.2.1 and reset the settings or make a new configuration.
2423 | 3.14.0.1 | 3.14.3.1 | If the profinet cloning is configured on the radio1, the system create the interface on the radio0. →Upgrade to 3.14.3.1.
2425 | 3.16.0.1 | 3.16.1.1 | The pin code is sent 2 time during the init. →Upgrade to 3.16.1.1.
2427 | 3.14.0.1 | 3.14.3.1 | The NTP client can have a synchronisation issue at startup. →Upgrade to 3.14.3.1.
2428 | 3.14.0.1 | 3.14.3.1 | On AirLink, EmbedAir the time zone is not configured correctly. →Upgrade to 3.14.3.1.
2443 | 3.14.0.1 | 3.14.3.1 | In some case the PIM deamon coud not start correctly. →Upgrade to 3.14.3.1.
2444 | 3.14.0.1 | 3.14.3.1 | Update the wifi regulation domain for Qatar country. →Upgrade to 3.14.3.1.
2446 | 3.16.0.1 | 3.16.1.1 | The LTE/GNSS daemon crash if it use an empty sim slot. →Upgrade to 3.16.1.1.
2448 | 3.16.0.1 | 3.18.0.1 | When the GNSS is fixed, the date returned throught the snmp interface is always the same. →Upgrade to 3.18.0.1.
2464 | 3.16.0.1 | 3.18.1.1 | The user's default netmask in openvpn settings is not saved. →Set the user's default netmask or upgrade to 3.18.0.1.
2466 | 3.16.0.1 | 3.18.1.1 | The openvpn settings doesn't work with NAT configuration. →Upgrade to 3.18.0.1.
2470 | 3.16.1.1 | 3.18.1.1 | In the QOS tagging feature, the destination IP field of the rule is ignored. →Upgrade to 3.18.0.1.
2472 | 3.14.3.1 | 3.14.5.1 | In roaming case, if we didn't receive a probe response from the AP we will send a probe to the AP before the association. The association is make after a probe response timeout (200ms). this case occur on each roaming if we use a DFS channel. →Upgrade to 3.14.5.1.
2474 | 3.14.3.1 | 3.14.5.1 | The 802.11r feature is not enabled correctly. →Upgrade to 3.14.5.1.
2486 | 3.14.3.1 | 3.14.5.1 | In some case, on product with 2 or more WiFi cards, the regulatory domain can be not set properly. →Upgrade to 3.14.5.1.
2488 | 3.14.3.1 | 3.14.5.1 | It is not possible to set the log level when 2 or more AP were configured on the same WiFi card. →Upgrade to 3.14.5.1.
2501 | 3.16.1.1 | 3.18.0.1 | The IMSI/IMEI are not show if the LTE module is not connected. →Upgrade to 3.18.0.1.
2503 | 3.16.1.1 | 3.18.0.1 | The event settings web page show an error on the AirBox. →Upgrade to 3.18.0.1.
2532 | 3.14.5.1 | 3.18.0.1 | It is not possible to configure an AirLink V2 with the configuration file from AirLink V1. →Upgrade to 3.18.0.1.
2544 | 3.14.5.1 | 3.18.0.1 | it is possible to lost some configuration information on AirLink, EmbedAir, AirBox, RuggedAir, AirXroad. →Upgrade to 3.18.0.1.
2560 | 3.14.5.1 | 3.18.0.1 | The PIM-SM protocol is not enable in the kernel. The multicast routing does not work on AirLink, EmbedAir, AirBox, RuggedAir, AirXroad. →Upgrade to 3.18.0.1.
2560 | 3.14.5.1 | 3.18.0.1 | It is not possible to use a non RSA private key. →Upgrade to 3.18.0.1.
2574 | 3.15.5.1 | 3.18.1.1 | On Airlink, RuggedAir, EmbedAir1000, AirBox, it is not possible to use the ethernet interface with a link negotiated at 10 Mbps HD. →Upgrade to 3.18.1.1.
2575 | 3.18.0.1 | 3.18.1.1 | If we configure 2 roles on the same Wi-Fi radio, the status in status->network is wrong. →Upgrade to 3.18.1.1.
2581 | 3.18.0.1 | 3.18.1.1 | on AirBox, it is not possible to configure an event on the second digital output. →Upgrade to 3.18.1.1.

back to top

version 3.18.0.1 release notes Changes Log Known issues
WaveOS changes log, 18-October-2018
Software and documentation copyright © by Acksys, 2018 - all rights reserved