# ACKSYS WaveOS

Changes Log Known issues

## Release notes up to version 4.36.0.1

### Documentation

- A User's guide referenced DTUS070 provides information common to all products supported by WaveOS.
- Installation guides provide data specific to each product. They are written both in English and French.
- The WaveManager software helps configure and monitor Acksys's Wi-Fi products. It installs in English or French, and comes with online help in English.

Latest documentation and WaveManager versions are available from the Acksys website (www.acksys.com).

### Upgrading to version 4.x.x.x

- The version 4.8.0.1 introduces the MESH network support.
  The SAE support for mesh is not compatible with all previous versions. All peers must have the same WaveOS version to communicate with each other.
  Don't upgrade to version 4.14.0.1 from 3.x versions. Please use version 4.14.1.1.
- An issue has been identified in the WaveOs firmware 4.18.0.1/4.18.1.1/4.18.2.1 and 4.20.0.1/4.20.0.2/4.20.0.3 where a possible corruption of the password, used for product access, could occurs. This problem has been fixed from the release 4.22.2.1.
  Unfortunately, as the corrupted passwords could not be recovered, the new firmware automatically reset the password and then the user must enter a new one

### Upgrading to version 4.30.0.1 and higher

As part of the compliance process with the EN18031-1 standard, several cryptographic algorithms have been removed. While this enhances overall security, it may cause compatibility issues with previous versions. We strongly recommend testing the update in a controlled environment before deploying it in your production environment.

### Downgrading to version 3.x.x.x

If you absolutely need to downgrade to 3.x.x.x release, once the download-and-reboot process is finished, you must reset the unit to factory settings before reconfiguring and reusing it.
So it may be unadviseable to do a downgrade on the field.

## Changes Log

Version / date | Changes
--- | ---
4.36.0.1 17-Jun-2026 | bugs Fixes and improvement
CVE fixed : package zlib : CVE-2022-37434 package dnsmasq : from CVE-2020-25681 to CVE-2020-25687 CVE-2022-0934 CVE-2023-28450 CVE-2023-50387 package curl : CVE-2018-0500 CVE-2018-16840 CVE-2019-5481 CVE-2019-5482 CVE-2021-22946 CVE-2022-32221 CVE-2022-27782 CVE-2023-28319 package libopenssl : CVE-2025-15467 CVE-2024-6119 CVE-2019-0190 CVE-2025-69419 CVE-2025-69420 CVE-2025-69421 package busybox : CVE-2018-1000517 CVE-2018-1000500 CVE-2018-20679 Fixed : #5213,#5257,#5260, #5278,#5293,
4.34.0.1 6-May-2026 | bugs Fixes and improvement
Added : Allow SRCC on WiFi 2 radio. Allow configuring the default firewall acceptance policy through SNMP Allow modifying DDNS instance through SNMP Fixed : #5236,#5235,#5234 #5233,#5232,#5091 Known bugs: On the 6 GHz band, automatic channel selection may choose a non-PSC channel in AP mode. When the DDNS instance is disabled through SNMP, its status remains enabled in the web interface.
4.32.4.1 27-February-2026 | bugs Fixes
Fixed : #4995,#5051, #5052,#5073,#5117,#5118, #5129,#5168,#5173
4.32.3.1 23-January-2026 | bugs Fixes
Fixed : #4711,#4753,#5018,#5075, #5142,#5145
4.32.2.1 19-december-2025 | bugs Fixes
Fixed : #4858,#5047,#5048, #5099,#5063,#5113,#5126
4.32.1.1 7-nov-2025 | bugs Fixes and improvement
Added Option to configure a scheduled system reboot Fixed : #5049,#5039,#5034,#5021,#5000,#4945, #4919,#4854
4.32.0.1 17-oct-2025 | bugs Fixes and improvement
Improvement Hide PIN code for cellular radio in system log Enabled log sending to WaveManager (requires WaveManager 4.6.0.1 or later) Enabled roaming information reporting to WaveManager (requires WaveManager 4.6.0.1 or later) Fixed : #5025,#4923,#4973,#4816,#4748
4.30.0.1 12-sept-2025 | EN18031-1 standard compliance update
Removed: Removed insecure cryptographic algorithms from some packages Removed SNMPV1 support Removed WEP and WPA wifi policies Removed support of TLS 1.1 and 1.2 Added: Added secure upgrade mechanism Increased the password requirement Added parameters to control password requirement Upgraded: Upgraded ssh server Upgraped openVPN package Modifed web server: https by default for access to the build-in web UI The default firewall policy Fixed : #4889,#4750,#4763, ,#4795
4.28.7.1 14-april-2026 | bug fixes
Fixed : backport of fix #5278.
4.28.6.1 12-may-2025 | bug fixes
Fixed : #4716,#4709,#4684
4.28.5.1 14-march-2025 | bug fixes
Fixed : #4644,#4646
4.28.4.1 14-feb-2025 | bug fixes
Fixed : #4607
4.28.3.1 22-jan-2025 | bug fixes
Fixed : #4466,#4492, #4595
4.28.2.1 27-dec-2024 | fix and improvements
Add configuration file compatibility from Railbox/20 to Railbox/22 and Railbox/10 to railbox /11 Fixed : #4513,#4508, #4474
4.28.1.1 04-oct-2024 | fix
Fixed : #4442,#4447, #4452,#4453, #4454,#4455,#4457, #4461,#4463,#4464,
4.28.0.1 25-jul-2024 | improvement
Add log record on the RailboxV2 Add OID to configure AutoAPN Add OID to configure the personal cloud Allow to force the ethernet port setting (speed and duplex) Add support of Verizon network
4.26.1.1 19-jul-2024 | Bug fixes
Fixed : #4377,#4424
4.26.0.1 26-jun-2024 | Bug fixes and improvements
Add support of LLDP Add support of ItXPT (service inventory, GNSS, time) Add support of MQTT for telemetry service. Note : The acksys cloud require WaveManager version 4.4.0.1 or later Allow to crypt or not the EAPOL frame during WPA exchange IPsec : allow to remap IP on local network Fixed : #4198,#4260,#4346,#4373,#4383,#4389 Note : The fix for #4383, will increase the reboot delay just after the configuration file is loaded .
4.24.5.1 12-Apr-2024 | Bug fixes
Fixed #4334, #4362 OID for 11ax cards in the configPhyWifiTable .1.3.6.1.4.1.28097.8.2.1.1.20 : Allow to read/write the band use by the Wifi card. When the band is changed, the product will reboot .1.3.6.1.4.1.28097.8.2.1.1.21 : Allow to read/write the primary wide Segment. Use when the channel width is set to 80 ou 160 .1.3.6.1.4.1.28097.8.2.1.1.22 : Allow to read/write the secondary wide segment. use when the channel width is set to 80+80
4.24.4.1 29-Mar-2024 | Bug fixes
Fixed #4265, #4357, #4358, #4208, #4315
4.24.1.1 06-Mar-2024 | Bug fixes
Fixed #4062, #4262, #4320, #4323, #4328, #4330, #4342
4.24.0.1 31-Jan-2024 | Bug fixes and improvements
Improve PLH roaming algorithme uprade gpsd package Add configuration file compatibility from Railbox/DR V2 to Railbox/DS V2 Enable roaming features for WIFI5 and WIFI6 products upgrade VRRP package Fixed #4256, #4277, #4261, #4263, #4279, #4294, #4305, #4306
4.22.3.1 13-Oct-2023 | Bug fixes
Fixed #4247, #4196
4.22.2.1 03-Oct-2023 | Bug fixes And add cellular radio
Add Cellular radio supprt for railbox V2. Add support of coding S and V Fixed #4201, #4214, #4220, #4228, #4232 , #4236, #4238 Known bug : #4243
4.22.1.1 08-Aug-2023 | Bug fixes
Fixed #4197
4.22.0.1 17-jul-2023 | Bug fixes and improvements
Enable cellular card in default settings Enabled routing thought the cellular interface in default settins Add support of auto APN Disable default password for root user. Force to configure a password for root user Check the password strength Add automatic switch sim on metrics Add DDNS (Dynamic DNS) support Add support DHCPV6 in client and server mode Add support of SRCC on product with 11ax wifi card Add support of Ackys MIB version 3.20.0.1 Add list of service Add IPV6 status Add cellular switch sim informations Fixed #4120, #4140, #4154, #4157, #4177, #4189
4.20.3.1 24-feb-2023 | Bug fixes
Fixed #4110, #4117, #4118, #4119
4.20.2.1 08-feb-2023 | Bug fixes
Fixed #4097, #4098
4.20.1.1 01-feb-2023 | Bug fixes
Fixed #4087
4.20.0.1 27-jan-2023 | Improvements
Add support of RailboxV2 Add support of wifi6 (802.1111ax) cards
4.18.7.1 16-feb-2023 | Bug fixes
Fixed #4039, #4069
4.18.6.1 11-jan-2023 | Bug fixes
Fixed #4068
4.18.5.1 4-jan-2023 | Bug fixes
Fixed #3906, #3980, #4060, #4066
4.18.4.1 16-dec-2022 | Bug fixes
Fixed #4034, #4050,
4.18.3.1 28-oct-2022 | Bug fixes
Fixed #3983, #4007, #4010, #4015, #4029
4.18.2.1 14-oct-2022 | Bug fixes
Fixed #3957, #3984, #3985, #4000
4.18.1.1 23-sep-2022 | Bug fixes
Fixed #3950,#3963
4.18.0.1 27-jully-2022 | Bug fixes and improvements
Improve IPV6 support Add SLAAC support on all interfaces Add NAT6 support Add support of wifi bridge wifi IPV6 settings Add IPSEC support Modification of PLH feature to improve the AP selection Upgrade LibOpenSSL to version 1.1.1n fixed #3398,#3775,#3799,#3818,#3819,#3832,#3853,#3872,#3875,#3876,#3897,#3928
4.16.12.1 30-nov-2022 | SRCC fixes and enhancements
SRCC proper: Additional fix for #3957: During the "connection established" state, set an ICMP watchdog for layer 3 connectivity → first-level recovery disconnects and reconnects the wireless link; if first-level fails, second-level recovery restarts the device Additional fix for #3957: Track WPA decipher process and recover on excessive failures Rise broken link log to NOTICE on AP side Move srcc-created hostapd/supplicant logging to syslog Exchange backbone IP address with wireless peers Validate wireless messages more thoroughly Wait for better peers and always select best peer Fix #3979: propagate packets priority to wireless media Other: Fix #3957: hangup case on WPA rekeying GUI warning on excessive receive signal power
4.16.11.1 24-may-2022 | GUI setup enhancements
Display unavailable events with "unavailable" indication Set "temperature" event as unavailable for such products Tracker #3893
4.16.10.1 12-may-2022 | Bug fixes
fixed #3881
4.16.9.1 12-apr-2022 | Bug fixes
fixed #3863,#3864,
4.16.8.1 31-mar-2022 | Improvements
SRCC: Add legacy mode. This mode allow the user to force the usage of SRCC V1. This mode is automatically selected after upgrade from WaveOS wich only support SRCC V1
4.16.7.1 29-mar-2022 | Bug fixes and improvements
fixed #3833,#3847, #3848,#3849 SRCC V2: Improve compatibility with the V1, to avoid the fallback to V1 when the links is establish. Telemetry: Show in log the IP address of the connected equipement.
4.16.6.1 24-mar-2022 | Bug fixes
fixed #3844
4.16.5.1 18-mar-2022 | Bug fixes
fixed #3839,#3840
4.16.4.1 16-mar-2022 | Bug fixes
fixed #3837,#3838
4.16.3.1 15-mar-2022 | Bug fixes
fixed #3835,#3836
4.16.2.1 11-mar-2022 | Bug fixes
fixed #3821, #3823, #3824, #3827 #3828, #3829
4.16.1.1 25-feb-2022 | Bug fixes and improvements
Wireless Association Controller : Pull down some messages from DEBUG level to INFO level fixed #3814
4.16.0.1 14-feb-2022 | Bug fixes and improvements
Add IPV6 support Allow static IPV6 configuration for network Allow Radius serveur with IPV6 NTP client can use IPV6 to reach the server The builtin logger can send the log to an IPV6 log server Allow IPV6 routing and bridging Allow to check the filesystem integrity Allow Asynchronous sysupgrade. The user can schedule the upgrade time Allow ssh server settings from web interface Add rogue AP service. This service allow to detect Rogue AP Add MIB version 3.18.0.1 Add OID and trap for rogue AP service Add OID for filesytem integrity check service Add OI to set NT server Fixed #3782,#3770
4.14.2.1 14-jan-2022 | Bug fixes
fixed #3608,#3628,#3681,#3710, #3712,#3718,#3721,#3759, #3761,#3764,#3767,#3769, #3778
4.14.1.1 20-sept-2021 | Bug fixes
fixed #3631,#3651,#3683
4.14.0.1 02-Jul-2021 | Bug fixes and improvements
Add IPv6 SLAAC support for LTE interface Rebuild the OpenVPN web interface, to support new feature Allow to configure the producte date from the GPS Add OIDs to configure date and timezone from SNMP Add support of AirWan product range Improve Wac feature for the station below the roaming trigger Allow to customize the http/https service port Allow channel 144 for US region fixed #3235,#3308,#3430,#3549,#3552,#3575, #3577,#3581#3597,#3603,#3632
4.12.2.1 14-Apr-2021 | Bug fixes
fixed #3463,#3475,#3444,#3472,#3476
4.12.1.1 25-Mar-2021 | Bug fixes
fixed #3419,#3423,#3431,#3437,#3457
4.12.0.1 3-Feb-2021 | Bug fixes and improvements
Add WPA3 support Add HotSpot 2.0 (802.11u) support Passpoint support EAP-SIM/EAP-AKA authentication support Online signup support Add client load balancing for AP mode Band steering Client roaming control Add Predictive Linear Handover (PLH) roaming algorithm for CBB Add VRRP master management by SNMP event. SSL librairie upgrade. With this upgrade only TLS 1.1, 1.2 and 1.3 are supported. Please check the TLS version supported by your application (radius server, web browser, ...) before upgrade. Support MIB 3.14.0.1 Add OIDs for CBB and PLH status Add OIDs for Cellular configuration Add WPA3 support Add event support to trig action in product fixed #3406,#3410 known bugs #3419,#3431
4.10.1.1 12-Jan-2021 | Bug fixes
fixed #3264,#3275,#3396
4.10.0.1 12-oct-2020 | Bug fixes and improvements
Add support of 11ac wave2 Add support of NAT 1:1 Add support of telemetry feature (require WaveManager 2.10.0.1) Support MIB 3.12.0.1 Add OIDs to return roaming status fixed #3070,#3105,#3195,#3202, #3245,#3248,#3232,#3216
4.8.1.1 17-Aug-2020 | Bug fixes
fixed #3123,#3230
4.8.0.1 20-mar-2020 | Bug fixes and improvements
Add Connect Before Break feature Add support for LACP as bonding mode Add support for WaveNet-Ex product range Add MESH support for 802.11n radio Allow to give the PUK code from the web interface Support MIB 3.10.9.1 Add an OID to return channel width (HT mode) in scan result Allow to configure the anonymous identity for PEAP-MSCHAPV2 fixed #2842, #2939, #2996, #3018, #3072, #3094, #3097, #3099
4.4.5.1 28-feb-2020 | Bug fixes
fixed: #3017, #3084, #3085, #3050, #3051, #3090, #3093 Known bugs #2842 (MESH mode doesn't work)
4.4.4.1 13-dec-2019 | Bug fixes
fixed #3015 Known bugs #2842 (MESH mode doesn't work)
4.4.3.1 12-dec-2019 | Bug fixes
fixed #3007 Known bugs #2842 (MESH mode doesn't work)
4.4.2.1 14-nov-2019 | Bug fixes
This version is only for AirLink, AirBox, AirXroad, EmbedAir100, EmbedAir1000, RuggedAir100, RuggedAir1000 fixed #2999 Known bugs #2842 (MESH mode doesn't work)
4.4.1.1 08-nov-2019 | Bug fixes and improvements
Allows to always boot the product with WiFi disabled fixed #2938,#2943, Known bugs #2842 (MESH mode doesn't work)
4.4.0.1 09-oct-2019 | Bug fixes and improvements
Add bonding support on Ethernet port (mode broadcast and round robin) Use NTP server from DHCP lease fixed #2666,#2814,#2854, #2875,#2878,#2885,#2889, Known bugs #2842 (MESH mode doesn't work)
4.2.1.1 24-july-2019 | DFS channels fixes, log improvements
Saving configuration changes writes a message in the system log Several irrelevant warnings are removed from the system log Fix RailBox/11 specific issues: #2854, #2864 Known bugs #2814 (SRCC mode doesn't work) #2842 (MESH mode doesn't work)
4.2.0.1 05-july-2019 | Major version
updated update kernel version to 4.9.111 update wifi driver update wifi deamons added DHCP relay support 802.1x authentication port based SNMPV3: SHA-224, SHA-256, SHA-384, SHA-512 support for authentication SNMPV3: AES-192, AES-256 support for Encryption Password strength meter for WEB interface password Add log on WEB authentication fixed #2731,#2776,#2818, #2825,#2833 known bugs #2814 (SRCC mode doesn't work) #2842 (MESH mode doesn't work)
4.0.0.1 Not released | Development version
This version was not released.
3.18.4.1 25-Sep-2020 | Bugs fixes
Fix issue:#2818
3.18.3.1 02-Apr-2019 | Bugs fixes
Revert modification for request #2663. These modifications introduce an issue during the apply process. In fact in this case the deamon was not really hanged, in some case the apply config can take several minutes to apply all settings. Fix issues:#2684
3.18.2.1 06-Mar-2019 | Bugs fixes
Fix issues:#2663 Add fixes from 3.14.6.1 and 3.14.7.1 → Starting with this version, the following products are not supported anymore. Wln-Aboard range Wln-RailBox range Wln-xRoad V1
3.18.1.1 19-Nov-2018 | Bugs fixes and improvement
Improve the wifi enable/disable management in the web interface Fix issues:#2574, #2575, #2581 →This version does not contain fixes from version 3.14.6.1 and 3.14.7.1
3.18.0.1 17-Oct-2018 | Bug fixes and improvement
Add event-driven IP interface selection. That allows switching route between LTE, WiFi, Ethernet. SRCC: Allow the pre-shared key configuration Add AirXroad support Add RuggedAir range support Allow firmware upgrade for LTE card Allow to use a non RSA private Key Fix issues:#2448, #2464, #2466., #2470, #2501., #2503, #2532., #2544, #2560., #2561, #2562. →This version does not contain fixes from version 3.14.6.1 and 3.14.7.1
3.16.1.1 3-July-2018 | Bug Fixes and improvement
Add GNSS/LTE status in SNMP Support Acksys MIB 3.10.6.1 Add GNSS status Add LTE status Fix issues: #2425,#2446 →This version does not contain fixes from version 3.14.6.1 and 3.14.7.1
3.16.0.1 25-Apr-2018 | Improvement
Add AirBox support Add GNSS and LTE support. →This version does not contain fixes from version 3.14.6.1 and 3.14.7.1
3.14.7.1 9-Jan-2019 | Bug fixe
Fix issue:#2613 → Fixe is integrated in main branch in version 3.18.2.1
3.14.6.1 18-Dec-2018 | Bug fixes
Fix issues:#2472, #2584 → Fixes are integrated in main branch in version 3.18.2.1
3.14.5.1 30-Aug-2018 | Bug fixes
Fix issues:#2472, #2474, #2486, #2488.
3.14.3.1 02-July-2018 | Bug fixes and improvement
Fix issues:#2423, #2427, #2428, #2443, #2444. In roaming settings, force client disconnection on duration for min/max threshold
3.14.2.1 15-May-2018 | Bug fixes
Fix issues:#2409, #2413, #2416, #2417
3.14.1.1 18-Apr-2018 | Bug fixes
Fix issues:#2359, #2369, #2371, #2379, #2389, #2390, #2391, #2399, #2403
3.14.0.1 7-Mar-2018 | Improvements and bug fixes
Add "user" login account to show the product status. This login can't change/show the product settings. Add openVPN support (client and server) Update the Qatar regulatory domain Add parameter to allow the wifi client to send a deauthentication frame to the AP leaved Fix Key Reinstallation Attacks (KRACK) Support ACKSYS-MIB version 3.10.4.1 Add SAE (Mesh security) support Add product identification support Fix issues: #878,#1696,#1955, #2058,#2234,#2318,#2343
3.12.14.1 5-Feb-2018 | bug fix
Fix issue: #2319
3.12.13.1 5-Feb-2018 | bugs fixes
Fix issues: #2311, #2321
3.12.12.1 24-Nov-2017 | Improvement and bugs fixes
Fix issues: #2250, #2254, #2255, #2273, #2275 Add config status web page, to check the configuration. Add SRCC deamon status web page
3.12.11.1 16-Oct-2017 | Improvement and bug fixes
Fix issues: #2156, #2161 #2218, #2226 #2235 Add hostname option in DHCP settings Add DHCP information in status/network web page Add DNS server information in status/network web page
3.12.10.1 21-Sep-2017 | Improvements and bug fixes
Support ACKSYS-MIB version 3.10.3.1 Add srcc link status Fix issues: #2212, #2220 #2209, #2210
3.12.9.1 30-Aug-2017 | Improvements and bug fixes
Support ACKSYS-MIB version 3.10.2.1 Add Mesh survey table Add Input filter groups settings Add somes Wireless advanced settings Add SRCC settings Add input bridge filter Fix issues: #2164, #2165, #2182, #2183, #2189
3.12.8.1 12-july-2017 | Improvements and bug fixes
Upgrade Pim deamon. That fix some issues and improve the protocol performance. → WARNING: This upgrade is not compatible with the previous version. You must upgrade all products. Fix VRRP protocol management. That fix some issues (static route not applied, GRE tunnel not enable when VRRP is master, ...). → WARNING: With this fix it is not possible to have VRRP and DHCP protocol on the same network. Add persistence parameter in the advanced network settings. fix issues:#2095,#2141,#2144,#2150,#2151,#2154
3.12.7.1 16-june-2017 | Improvements and Bug Fixes
Reduction of packet loss on highest WMM QOS in case of network congestion: #2063 Add EmbedAir 1000 products range support Add onlink parameter in static routes settings Fix issues: #2116,#2097
3.12.6.1 30-may-2017 | Improvements and Bug Fixes
Roaming improvements: #2061,#2096,#2112 Enable routing in L25NAT mode with local router: #2098 Fix issues: #2109
3.12.5.1 22-may-2017 | Improvement
Support of WaveManager Version 1.0.0.0
3.12.4.1 11-may-2017 | Bug Fixes
Fix issues: #2086,#2087
3.12.3.1 04-may-2017 | Improvements and Bug Fixes
Support ACKSYS-MIB version 3.10.0.1 Add some OID for network status Add an OID to return the hash result of the configuration Add OID to allow a binary file transfert to the product Update remote access security for advanced users Fix issues: #2049,#2051, #2056,#2057,
3.12.2.1 13-Apr-2017 | Improvements and Bug Fixes
Configuration of buffer size for power saving stations in the AP Fix issues: #2012,#2023, #2031,#2036, #2042,#2044, #2045,#2046, #2047,
3.12.0.1 16-Mar-2017 | Improvements and Bug Fixes
Management of VLAN priority on 802.1Q VLAN interfaces Set localhost and ip destination to firewall rules Adding source ip field to firewall rules Adding frame protocol GRE to firewall rules Adding sort of the firewall rules VRPP: Add unicast peer for Advertisement VRRP: Add multicast group settings Add EmbedAir range products support Support Acksys MIB version 3.8.8.1 Add WiFi association table Add wired Ethernet interface status Add DFS channel support on mesh mode Management of GRE endpoints on VRRP virtual addresses Fixing VRRP virtual IP loss by virtual VLAN interfaces after link down then link up Deleting GRE static route from configuration after Gre interface deletion from config file Fix issues: #1629, #1948,#1963, #1992,#1996, #1951, #2005,#2007,
3.10.2.1 31-jan-2017 | Bug Fixes
Fix issue #1946
3.10.1.1 16-jan-2017 | Bug Fixes
Management of VLAN interfaces on Wifi interfaces with Client STA roles Fix issue #1910 Fix issue #1911
3.10.0.1 13-dec-2016 | Bug Fixes and MIB improvement
Support ACKSYS-MIB version 3.8.6.1 Add 802.11ac settings Add Wifi multichannel management Add GRE settings Add Roaming settings Add network friendly name Add gateway in network settings Allow to set a bridge on network settings Allow to show the WPA preshared key with SNMP V3 in default settings Improvement WPA security management Bug Fixes on somes OID Fix IP format error in somes OID Improve the status Association list in product web page Improve the SRCC log message Update SSL library to fix some security issue Fix issue #1727,#1826,#1841,#1846, #1856,#1863,#1875,#1887
3.8.0.1 14-oct-2016 | Bug Fixes and Wln range support
Add WLn range support Support ACKSYS-MIB version 3.8.5.1 Add OID to download the WPA user certificat Add OID to configure the DNS relay Add OID to set the WPA key life time Add OID to set the off-channel delay for the active scan in roaming mode Add OID to know the RSTP status Add Discover agent password setting Clonning: Add Pre-connect feature Add support HT40 automatic for client mode Fix issue #1432,#1553,#1719,#1721, #1768,#1774,#1787
3.6.0.1 23-July-2016 | Bug Fixes and improvement
Add PIMd support SRCC: Allow tx power settings SRCC: Send log to product syslog Add static clonning support Add IP alias settint Add bandwith tools in Web interface Add spectral analyzer for 11n card Add graphical view of WiFi scan Add wifi service status Add SNMP V3 OID to enable/disable ssh server Fix issue #1591,#1663,#1677,#1685
3.4.2.1 12-Apr-16 | Bug Fixes and improvement
Fix issue #1637 : If the password file is corrupted, the upgrade will close the web access for security reason. You must restore the factory settings and restore your settings. Add RSTP daemon monitoring.
3.4.1.1 22-Mar-16 | RSTP improvement
Improve the RSTP link down detection on the wireless interface when she is overload.
3.4.0.1 09-Mar-16 | Bug fixes and Firmware improvements
Add VRRP support. Add SRCC mixed redundant mode: Add redundant coupling topology with 1 wired link and WiFi link. MCS list configuration: On RailBox/11, allow to set the MCS list supported by the AP. Add SNMP V3 support Managed settings compatibility with WLn series Add bandwith graphics in Web Interface Fix issues #1481,#1506,#1537,#1543,#1555 ,#1562,#1568
3.2.0.1 27-Nov-15 | First WaveOS release
QOS support : QOS supports up to 7 priority levels. Shares the availabe priority level bandwidth between all streams. SRCC support : Automatic solution for the carriage coupling. RSTP support: Rapid Spaming Tree allows ring network topoligy and redundant network. L2 GRE tunnel support Support VLAN in the bridge Disable WiFi service if network host does not respond to the ping Send trap when DFS event occurs

back to top

## ACKSYS WaveOS known issues

Please note that several problems reported to our technical support were found as customer problems or non-bugs, thus the holes in the numbered list below.
When provided, countermeasures apply until the issue is closed.

Tracker# | found in versions | version corrected | Description / Countermesures
--- | --- | --- | ---
878 | 3.0.0.1 | 3.14.0.1 | The OID statusPhyWifiScanTableUpdateTbl may return 'Available' when the scan is finished. →Update to 3.14.0.1
1432 | 3.2.0.1 | 3.8.0.1 | With some web browser, it can be impossible to commit the wireless settings. →Update to 3.8.0.1
1480 | 3.2.0.1 |  | It is not possible to send VLAN tagged frames through the WiFi interface. →use L2 GRE tunnel on wireless interface if you need to send VLAN tagged frames.
1481 | 3.2.0.1 | 3.4.0.1 | On RailBox/11, the connection between the AP and the sta can be dropped during the WPA rekeying. →Set the rekeying delay to 0.
1506 | 3.2.0.1 | 3.4.0.1 | On RailBox/11, the SAE security doesn't work. →Upgrade to 3.4.0.1
1537 | 3.2.0.1 | 3.4.0.1 | The frame filter on GRE interface doesn't work.
1543 | 3.2.0.1 | 3.4.0.1 | The wireless clonning mode doesn't work
1553 | 3.2.0.1 | 3.8.0.1 | In some cases, it is possible to have an incomplete GRE tunnel configured, and it is not possible to delete it.
1555 | 3.2.0.1 | 3.4.0.1 | If the bridge VLAN feature is enabled on the bridge and a wireless interface is added in the bridge and the wireless interface uses the automatic channel select or DFS channel, the bridge VLAN settings are not applied.
1562 | 3.2.0.1 | 3.4.0.1 | The administrator password is not exported in the C-KEY nor the configuration file.
1568 | 3.2.0.1 | 3.4.0.1 | The wireless "g only" mode is not compatible between the WLg and Railbox series. →Use the "b/g" mode instead.
1591 | 3.4.0.1 | 3.6.0.1 | Access to the web interface with HTTPS protocol doesn't work. →Upgrade to 3.6.0.1
1629 | 2.8.0.1 | 3.12.0.1 | The scan result get from snmp, the latest mac address byte is missing. →Upgrade to 3.12.0.1
1637 | 3.4.0.1 | 3.4.2.1 | If the password file is corrupted, the web interface access is not protected. The password can be corrupted if you change the password and power off the product, while the modifications are saved. →Upgrade to 3.4.2.1
1663 | 3.0.0.1 | 3.6.0.1 | The https server is vulnerable to several SSL attack (Hearthbleed, CCS injection, Poodle, ...). →Upgrade to 3.6.0.1
1677 | 3.0.0.1 | 3.6.0.1 | The settings backup file list are not the same between the C-Key and the web interface backup. →Upgrade to 3.6.0.1
1685 | 3.4.2.1 | 3.6.0.1 | the "Wireless/channel status" web page is not available. →Upgrade to 3.6.0.1
1696 | 3.5.0.1 | 3.14.0.1 | The OID internalAlarmSwitch doesn't return the Switch status →Upgrade to 3.14.0.1
1719 | 3.6.0.1 | 3.8.0.1 | In some cases, it is possible to have an internal error on Vlan bridge settings. →Upgrade to 3.8.0.1
1721 | 3.4.0.1 | 3.8.0.1 | Wireless mesh mode is not compatible with DFS. Add check in the wireless settings →Upgrade to 3.8.0.1
1727 | 3.0.0.1 | 3.10.0.1 | If the GRE local IP is not reachable when the GRE is initialized, all GRE traffic are send to the gateway. →Upgrade to 3.10.0.1
1768 | 3.6.0.1 | 3.8.0.1 | In setup/physical interfaces overview, one error occur if the user select several channels in interface settings. →Upgrade to 3.8.0.1
1774 | 3.6.0.1 | 3.8.0.1 | The MCS list is not generated on RailBox/21 and RailBox/25 →Upgrade to 3.8.0.1
1787 | 3.6.0.1 | 3.8.0.1 | If the user change the product time zone, the product stay in UTC time zone. →Upgrade to 3.8.0.1
1826 | 3.6.0.1 | 3.10.0.1 | In some cases the SRCC association can failed or is slow. →Upgrade to 3.10.0.1
1841 | 3.8.0.1 | 3.10.0.1 | On Wln platform, the graphical bandwidth report doesn't work. →Upgrade to 3.10.0.1
1846 | 3.8.0.1 | 3.10.0.1 | If the 802.11w is enable on the AP, it is doesn't work correctly. →Upgrade to 3.10.0.1
1856 | 3.8.0.1 | 3.10.0.1 | In setup/physique interface page the filters group link doesn't work.
1863 | 3.6.0.1 | 3.10.0.1 | The timezone settings is not correctly applied. →Upgrade to 3.10.0.1
1875 | 3.6.0.1 | 3.10.0.1 | The access to the page status wirless is not possible if all wireless card are disabled
1887 | 3.8.0.1 | 3.10.0.1 | With chrome version 55 some web page are not showed corretly. →Upgrade to 3.10.0.1
1910 | 3.10.0.1 | 3.10.1.1 | The mesh SAE security don't work correctly with another WaveOS version. →Upgrade to 3.10.1.1
1911 | 3.10.0.1 | 3.10.1.1 | It is not possible to create an VLAN Virtual interface on Wifi interface on mesh. →Upgrade to 3.10.1.1
1946 | 3.10.0.1 | 3.10.2.1 | If you use SRCC on wifi 1 and AP on wifi 2, on certainly case the AP on wifi 2 can be disable during the SRCC association. →Upgrade to 3.10.2.1
1948 | 3.11.0.5 | 3.11.0.51 | snmpd: fix engineID management →Upgrade to 3.11.0.51
1951 | 3.10.0.1 | 3.12.0.1 | In the web server, when the site survey is finished, in certainly case we don't see the result but we are redirected to the home page. →Upgrade to 3.12.0.1
1955 | 3.11.0.1 | 3.14.0.1 | It is not possible to change the Radius port in WPA/WPA2 settings. →Upgrade to 3.14.0.1
1963 | 3.11.0.5 | 3.11.0.51 | Fix snmpd agent version v3 value →Upgrade to 3.11.0.51
1992 | 3.10.0.1 | 3.12.0.1 | When the product is upgraded with NDM, the upgrade result from the product is "saving config files". →Upgrade to 3.12.0.1
1996 | 3.10.0.1 | 3.12.0.1 | In certanly case, the product can crash after several VRRP switch over. →Upgrade to 3.12.0.1
2005 | 3.10.0.1 | 3.12.0.1 | When the VRRP logs are enabled, some time the product can crash. →Upgrade to 3.12.0.1
2007 | 3.10.0.1 | 3.12.0.1 | In multicast routing, if the query interval is set to a value higher than 46s, the multicast routing can stop randomly. →Upgrade to 3.12.0.1
2012 | 3.12.0.1 | 3.12.2.1 | Fix system hanging during boot in some rare conditions. →Upgrade to 3.12.2.1
2023 | 3.12.0.1 | 3.12.2.1 | Fix antennas choice list. →Upgrade to 3.12.2.1
2031 | 3.12.0.1 | 3.12.2.1 | Certain advanced mesh parameters are not working properly. →Upgrade to 3.12.2.1
2036 | 3.12.0.1 | 3.12.2.1 | 5GHz channels must not be usable in Israel. →Upgrade to 3.12.2.1
2042 | 3.12.0.1 | 3.12.2.1 | Can not configure bridge broadcast filter per snmp. →Upgrade to 3.12.2.1
2044 | 3.12.0.1 | 3.12.2.1 | Bridge filter is not working. →Upgrade to 3.12.2.1
2045 | 3.12.0.1 | 3.12.2.1 | Bridge filter rules are not applied on Ethernet port after a reboot. →Upgrade to 3.12.2.1
2046 | 3.12.0.1 | 3.12.2.1 | Error when displaying traffic class prio status page. →Upgrade to 3.12.2.1
2047 | 3.12.0.1 | 3.12.2.1 | SSIDs of wifi interfaces are not displayed in QOS traffic class prio submenu. →Upgrade to 3.12.2.1
2049 | 3.12.0.1 | 3.12.3.1 | In SRCC, the link establishement can be too long. →Upgrade to 3.12.3.1
2051 | 3.12.0.1 | 3.12.3.1 | In certainly case the discover service response can be not correct. The NDM view can be affected. →Upgrade to 3.12.3.1
2056 | 3.12.0.1 | 3.12.3.1 | If the bridge VLAN feature is enable and all bridge ports don't participate to the sames VLAN, some communication can not work correctly. This bug only affect the RailBox products. →Upgrade to 3.12.3.1
2057 | 3.12.0.1 | 3.12.3.1 | The bridge filter configuration through SNMP, can return some default values. These values are not writen in the configuration file. →Upgrade to 3.12.3.1
2058 | 3.12.0.1 | 3.14.0.1 | Somes OID return the default value even if the value was not set. →Upgrade to 3.14.0.1
2086 | 3.12.3.1 | 3.12.4.1 | In certainly case it is not possible to set the client mode throught the Web interface. The interface return an error during the save process. →Upgrade to 3.12.4.1
2087 | 3.12.3.1 | 3.12.4.1 | A buffer overflow can occure in Acksys Mib library. The result is some no consistant information is returned by the SNMP interface. →Upgrade to 3.12.4.1
2061 | 3.12.4.1 | 3.12.6.1 | Roaming improvement with multiple Vlans topology →Upgrade to 3.12.6.1
2096 | 3.12.4.1 | 3.12.6.1 | Reduction of packet loss during roaming →Upgrade to 3.12.6.1
2098 | 3.12.4.1 | 3.12.6.1 | Enable routing in L25NAT mode with local router →Upgrade to 3.12.6.1
2109 | 3.12.4.1 | 3.12.6.1 | Fix wrong status showed in NDM during roaming →Upgrade to 3.12.6.1
2112 | 3.12.4.1 | 3.12.6.1 | Roaming: Add parameter to control station deauthentication →Upgrade to 3.12.6.1
2063 | 3.12.6.1 | 3.12.7.1 | Reduction of packet loss on highest WMM QOS in case of network congestion →Upgrade to 3.12.7.1
2097 | 3.12.6.1 | 3.12.7.1 | Fix: VRRP stops sending advertisements on an interface after that it has roamed. →Upgrade to 3.12.7.1
2116 | 3.12.6.1 | 3.12.7.1 | VRRP: Fix initialisation issue →Upgrade to 3.12.7.1
2095 | 3.12.2.1 | 3.12.8.1 | Multicast stream doesn't resume after the VRRP master reboot. →Upgrade to 3.12.8.1
2141 | 3.12.5.1 | 3.12.8.1 | The product ID used by NDM/WaveManeger is stored on configuration file and restored during the restore configuration process. If you restore a configuration on a product from another product, NDM, WaveManager will consider the both product as the same product. →Upgrade to 3.12.8.1
2144 | 3.12.7.1 | 3.12.8.1 | Firewall rules without src and dest zone are not displayed in the web interface. →Upgrade to 3.12.8.1
2150 | 3.12.5.1 | 3.12.8.1 | If network loop occure between the product network interface, an kernel crash occurs. →Upgrade to 3.12.8.1
2151 | 3.12.0.1 | 3.12.8.1 | Wifi regulation domain: The chile was changed the regulation rule. Update the regulation domain to respect the new rules. →WARNING: This upgrade will reduce the Txpower to 17dBm on band 5735 - 5835 MHz.
2154 | 3.12.0.1 | 3.12.8.1 | SNMP: Fix some OID to allow router configuration. →Upgrade to 3.12.8.1
2156 | 3.12.0.1 | 3.12.11.1 | SRCC: If the user select a chanel not compatible with the HT40+ mode, SRCC doesn't work →Upgrade to 3.12.11.1
2161 | 3.12.5.1 | 3.12.9.1 | The mono-card repeater doesn't work. →Upgrade to 3.12.9.1
2164 | 3.12.5.1 | 3.12.9.1 | VRRP and static route: If the product have a static route and ip alias, after two VRRP transition (the product back in backup) static route is not correctly set and it is not possible to access at the product from far network. →Upgrade to 3.12.9.1
2165 | 3.12.7.1 | 3.12.9.1 | The roaming log level doesn't show the roaming log. →Upgrade to 3.12.9.1
2182 | 3.10.0.1 | 3.12.9.1 | We can set an IP address with an invalide format wihtout Error in the web page. eg: 192.168.010.20 is invalide because the digit '010' is an octal représentation and it is not supported by the firmware. →Upgrade to 3.12.9.1
2183 | 3.12.0.1 | 3.12.9.1 | In NAT router configuration, some frames can be sent with the ip source set to an private IP. →Upgrade to 3.12.9.1
2189 | 3.12.0.1 | 3.12.9.1 | The bridge filter rules are not correctly applied on Wifi interface in AP mode configured to use a DFS channel. →Upgrade to 3.12.9.1
2209 | 3.12.0.1 | 3.12.1.1 | In snmp statusIfWlanTable, each wlan is present two times. →Upgrade to 3.12.10.1
2210 | 3.10.0.1 | 3.12.10.1 | The association counter (statusIfWlanPeers) don't work in mesh node. →Upgrade to 3.12.10.1
2212 | 3.12.9.1 | 3.12.10.1 | If two vrrp instance are configured in the same network, only one IP is applied. →Upgrade to 3.12.10.1
2218 | 3.12.9.1 | 3.12.11.1 | On EmbedAir and Airlink the WPA and WEP doesn't work. →Upgrade to 3.12.11.1 or use WPA2
2220 | 3.10.0.1 | 3.12.10.1 | In rarely case, the snmp deamon management can generate a configuration corruption. →Upgrade to 3.12.10.1
2226 | 3.12.7.1 | 3.12.11.1 | Fix product hanging in power save mode. →Upgrade to 3.12.11.1
2234 | 3.12.9.1 | 3.14.0.1 | The OID statusIpSubnetMenber from statusIpSubnetTable doesn't not give the list of interface member. →Upgrade to 3.14.0.1
2235 | 3.12.9.1 | 3.12.11.1 | The AP default settings are not the same in SNMP and Web interface →Upgrade to 3.12.11.1 or change the values after the AP is added with the SNMP interface.
2250 | 3.12.11.1 | 3.12.12.1 | The status network web page doesn't work (error 500) if one wifi card is disabled. →Upgrade to 3.12.12.1 or enable all wifi cards on the product.
2254 | 3.12.11.1 | 3.12.12.1 | The multicast routing deamon doens't work correctly when several IP address are set on managed interface. →Upgrade to 3.12.12.1.
2255 | 3.12.11.1 | 3.12.12.1 | The firewall and VRRP configuration files are not well synchronised with network configuration file. →Upgrade to 3.12.12.1.
2273 | 3.10.0.1 | 3.12.12.1 | The wireless status files can be corrupted. →Upgrade to 3.12.12.1 or reset to factory the settings.
2275 | 3.12.11.1 | 3.12.12.1 | The VRRP deamon is not properly stopped when the configuration is reloaded. →Upgrade to 3.12.12.1.
2311 | 3.12.11.1 | 3.12.13.1 | In WiFi client mode, If we received a Deauthentication frame from the AP the client will black list tis AP. In certainly case this list is not purged and the APs is not available for new association. →Upgrade to 3.12.13.1.
2321 | 3.12.11.1 | 3.12.13.1 | The Atheros Adaptive noise imunity doesn't work correctly. This fix can increase the Wifi performance in case of noisy environment. →Upgrade to 3.12.13.1.
2318 | 3.12.12.1 | 3.14.0.1 | The NTP client mays send the request before the interface is ready to forward the data. In this case the time synchronisation will perform on the next update. →Upgrade to 3.14.0.1
2319 | 3.12.12.1 | 3.12.14.1 | In WiFi roaming client mode, a wrong RSSI is sometimes obtained from the Access Points which use a DFS channel. This may result in incorrect selection of the Best AP to roam to. →Upgrade to 3.12.14.1 or, →Reduce the beacon interval on all relevant AP's to less than 70 ms (or 70 TU)
2343 | 3.12.11.1 | 3.14.0.1 | The page status/wireless/assoc in web server may not display →Upgrade to 3.14.0.1.
2359 | 3.14.0.1 | 3.14.1.1 | The web page to show the statistic graph show error and crash on wifi interface. →Upgrade to 3.14.1.1.
2369 | 3.14.0.1 | 3.14.1.1 | On the EmbedAir1000 it is not possible to configure an AP in 802.11ac mode. →Upgrade to 3.14.1.1.
2371 | 3.14.0.1 | 3.14.1.1 | In certainly case the signal level in client scan result is egal to 0. →Upgrade to 3.14.1.1.
2379 | 3.12.10.1 | 3.14.1.1 | In SRCC configuration, if the link is broken, it will be never restablished. →Upgrade to 3.14.1.1.
2389 | 3.14.0.1 | 3.14.1.1 | In system log if the line is too long that can store a line with some garbage. →Upgrade to 3.14.1.1.
2390 | 3.12.13.1 | 3.14.1.1 | If we configure an AP with pre-authentication in some case this feature is not enabled on the AP. →Upgrade to 3.14.1.1.
2391 | 3.14.0.1 | 3.14.1.1 | in mono-channel roaming configuration, the foreground scan doesn't work properly. →Upgrade to 3.14.1.1.
2399 | 3.14.0.1 | 3.14.1.1 | On RaiBox/RailTrack Ethernet interface Transmit fifo can overflow and occurs some packet lost. →Upgrade to 3.14.1.1.
2403 | 3.10.0.1 | 3.14.1.1 | In case of the configuration is restored from the C-KEY after an reset to factory settings, the network configuration stay in default settings. →Upgrade to 3.14.1.1.
2409 | 3.12.7.1 | 3.14.2.1 | If the product is set in DHCP mode, in Wifi client mode and bridging mode in ARPNAT, the product will reboot each time it should renew the DHCP lease. →Upgrade to 3.14.2.1 or use the WDS bridging mode (not compatible with roaming).
2413 | 3.14.0.1 | 3.14.2.1 | The status page status/wireless/services_status will generate an error in syslog. →Upgrade to 3.14.2.1.
2416 | 3.14.0.1 | 3.14.2.1 | If the product is set in DHCP mode, in Wifi client mode and bridging mode in ARPNAT, the checksum is wrong in the first renew frame sent. The renew at half lease dont' work properly. →Upgrade to 3.14.2.1.
2417 | 3.14.1.1 | 3.14.2.1 | The factory settingss on RailBox is wrong. The ip address is set to 192.168.1.1 and only LAN1 is in the default bridge. →Upgrade to 3.14.2.1 and reset the settings or make a new configuration.
2423 | 3.14.0.1 | 3.14.3.1 | If the profinet cloning is configured on the radio1, the system create the interface on the radio0. →Upgrade to 3.14.3.1.
2425 | 3.16.0.1 | 3.16.1.1 | The pin code is sent 2 time during the init. →Upgrade to 3.16.1.1.
2427 | 3.14.0.1 | 3.14.3.1 | The NTP client can have a synchronisation issue at startup. →Upgrade to 3.14.3.1.
2428 | 3.14.0.1 | 3.14.3.1 | On AirLink, EmbedAir the time zone is not configured correctly. →Upgrade to 3.14.3.1.
2443 | 3.14.0.1 | 3.14.3.1 | In some case the PIM deamon coud not start correctly. →Upgrade to 3.14.3.1.
2444 | 3.14.0.1 | 3.14.3.1 | Update the wifi regulation domain for Qatar country. →Upgrade to 3.14.3.1.
2446 | 3.16.0.1 | 3.16.1.1 | The LTE/GNSS daemon crash if it use an empty sim slot. →Upgrade to 3.16.1.1.
2448 | 3.16.0.1 | 3.18.0.1 | When the GNSS is fixed, the date returned throught the snmp interface is always the same. →Upgrade to 3.18.0.1.
2464 | 3.16.0.1 | 3.18.1.1 | The user's default netmask in openvpn settings is not saved. →Set the user's default netmask or upgrade to 3.18.0.1.
2466 | 3.16.0.1 | 3.18.1.1 | The openvpn settings doesn't work with NAT configuration. →Upgrade to 3.18.0.1.
2470 | 3.16.1.1 | 3.18.1.1 | In the QOS tagging feature, the destination IP field of the rule is ignored. →Upgrade to 3.18.0.1.
2472 | 3.14.3.1 | 3.14.5.1 | In roaming case, if we didn't receive a probe response from the AP we will send a probe to the AP before the association. The association is make after a probe response timeout (200ms). this case occur on each roaming if we use a DFS channel. →Upgrade to 3.14.5.1.
2474 | 3.14.3.1 | 3.14.5.1 | The 802.11r feature is not enabled correctly. →Upgrade to 3.14.5.1.
2486 | 3.14.3.1 | 3.14.5.1 | In some case, on product with 2 or more WiFi cards, the regulatory domain can be not set properly. →Upgrade to 3.14.5.1.
2488 | 3.14.3.1 | 3.14.5.1 | It is not possible to set the log level when 2 or more AP were configured on the same WiFi card. →Upgrade to 3.14.5.1.
2501 | 3.16.1.1 | 3.18.0.1 | The IMSI/IMEI are not show if the LTE module is not connected. →Upgrade to 3.18.0.1.
2503 | 3.16.1.1 | 3.18.0.1 | The event settings web page show an error on the AirBox. →Upgrade to 3.18.0.1.
2532 | 3.14.5.1 | 3.18.0.1 | It is not possible to configure an AirLink V2 with the configuration file from AirLink V1. →Upgrade to 3.18.0.1.
2544 | 3.14.5.1 | 3.18.0.1 | it is possible to lost some configuration information on AirLink, EmbedAir, AirBox, RuggedAir, AirXroad. →Upgrade to 3.18.0.1.
2560 | 3.14.5.1 | 3.18.0.1 | The PIM-SM protocol is not enable in the kernel. The multicast routing does not work on AirLink, EmbedAir, AirBox, RuggedAir, AirXroad. →Upgrade to 3.18.0.1.
2560 | 3.14.5.1 | 3.18.0.1 | It is not possible to use a non RSA private key. →Upgrade to 3.18.0.1.
2574 | 3.15.5.1 | 3.18.1.1 | On Airlink, RuggedAir, EmbedAir1000, AirBox, it is not possible to use the Ethernet interface with a link negotiated at 10 Mbps HD. →Upgrade to 3.18.1.1.
2575 | 3.18.0.1 | 3.18.1.1 | If we configure 2 roles on the same Wi-Fi radio, the status in status->network is wrong. →Upgrade to 3.18.1.1.
2581 | 3.18.0.1 | 3.18.1.1 | on AirBox, it is not possible to configure an event on the second digital output. →Upgrade to 3.18.1.1.
2584 | 3.14.5.1 | 3.14.6.1, >3.18.1.1 | Wi-Fi client roaming option "Do not cache old scan results" has not effect in radio cluster mode. →Upgrade to fixed version.
2613 | 3.14.5.1 | 3.14.7.1 | In some case, GRE interface is destroyed and multicast routing fails. →Upgrade to 3.14.7.1
2663 | 3.14.6.1 | 3.18.2.1 | If the network settings were changed, and the save and apply command is sent from SNMP interface, the SNMP deamon hang. After this action, it is not possible to reach the product through the SNMP interface. →Upgrade to 3.18.2.1
2666 | 3.18.1.1 | 4.4.0.1 | In some case, if the AP is configured in HT40 it can work in HT20. →Upgrade to 4.4.0.1
2684 | 3.18.2.1 | 3.18.3.1 | In some cases (dependent on the configuration files) when an application read the OID ConfigIpSubnet the snmp deamon crash. →Upgrade to 3.18.3.1
2731 | 3.14.1.1 | 4.2.0.1 | the snmp scan with the OID .1.3.6.1.4.1.28097.7.4 doesn't work correctly →Upgrade to 4.2.0.1
2776 | 3.14.1.1 | 4.2.0.1 | The default log level is set to "no log" for wifi deamons. This level does not allow to show the basic connection errors. Set the default log level to "info" for sta deamon. →Upgrade to 4.2.0.1
2814 | 4.0.0.1 | 4.4.0.1 | SRCC doesn't work →Upgrade to 4.4.0.1
2818 | 3.18.3.1 | 3.18.4.1 4.2.0.1 | If the engineID is set to motherboard ID, the engine ID is still the same on all products. →Upgrade to 3.18.4.1 or 4.2.0.1 and reselect the option.
2825 | 3.14.6.1 | 4.2.0.1 | In the roaming with cluster mode scan, the product may reboot. →Upgrade to 4.2.0.1
2833 | 3.18.3.1 | 4.2.0.1 | If the ntp server is not reachable for 60s, the ntpclient service is stopped. →Upgrade to 4.2.0.1
2842 | 4.0.0.1 |  | MESH mode doesn't work →upgrade to 4.8.0.1
2854 | 4.2.0.1 | 4.2.1.1 | On DFS channels, detection of some short pulses from radars fails. →Upgrade to 4.2.1.1
2864 | 4.2.0.1 | 4.2.1.1 | On DFS channels, radars detection brings up many false positives, resulting in the Access Point service going to the "DFS-NOP" state (visible in the web interface). →Upgrade to 4.2.1.1
2875 | 4.2.0.1 | 4.4.0.1 | If the user password is wrong, the web interface shows an error message. →Upgrade to 4.4.0.1
2878 | 4.2.0.1 | 4.4.0.1 | The time to read some OID is very long. →Upgrade to 4.4.0.1
2885 | 4.0.0.1 | 4.4.0.1 | in roaming condition, the scan frames are not always sent. This result in an incomplete scan result. →Upgrade to 4.4.0.1
2889 | 4.0.0.1 | 4.4.0.1 | in roaming condition, if a large bandwith is sent in the QOS level VO, the client disconnects. →Upgrade to 4.4.0.1
2938 | 4.4.0.1 | 4.4.1.1 | Parameters "Maximum time above maximum level" and "Maximum time under minimum level" are no longer visible in the WEB interface (but if they were defined before upgrade to 4.4.0.1, they remain valid). The correction makes them visible again. →Upgrade to 4.4.1.1
2939 | 4.4.0.1 | 4.8.0.1 | In client mode (without roaming) if you select several channels, the client still scan all channels. →Upgrade to 4.8.0.1
2943 | 4.4.0.1 | 4.4.1.1 | If the WiFi interface is not selected in the network named "LAN", it is not possible to set the LAN network IP via WaveManager. →Upgrade to 4.4.1.1
2996 | 4.4.0.1 | 4.8.0.1 | The GPS coordinates are not accurate from SNMP interface →Upgrade to 4.8.0.1
2999 | 4.4.1.1 | 4.4.2.1 | The setup->physical interface web page is not displayed correctly. An error prevents the Wi-Fi configuration. →Upgrade to 4.4.2.1
3007 | 4.4.0.1 | 4.4.3.1 | The dhcp Server may not start after a reboot, or may be stopped soon after. →Upgrade to 4.4.3.1
3015 | 4.4.3.1 | 4.4.4.1 | Sometimes the network service does not work at product startup. →Upgrade to 4.4.4.1
3017 | 4.4.4.1 | 4.4.5.1 | In some cases, the web page to configure the cellular return an error 500. →Upgrade to 4.4.5.1
3018 | 4.4.4.1 | 4.8.0.1 | In some cases, in the web interface, it is not possible to add firewall zone. →Upgrade to 4.8.0.1
3050 | 4.4.0.1 | 4.4.5.1 | The SNMP service stops working if the cellular interface is enabled and no SIM card is present. →Upgrade to 4.4.5.1
3051 | 4.4.0.1 | 4.4.5.1 | From SNMP interface, the IP configuration for cellular interface is always set to none. →Upgrade to 4.4.5.1
3070 | 4.4.0.1 | 4.10.0.1 | When a static route it use with the VPN service, the static routes are not applied in all cases. →Upgrade to 4.10.0.1
3072 | 4.4.0.1 | 4.8.0.1 | In SNMP interface, The oid ifIndex of the table statusIPSubnetTable can return a random value if the interface is down. →Upgrade to 4.8.0.1
3084 | 3.18.3.1 | 4.4.5.1 | On cellular product, it's impossible to use SIM 2. →Upgrade to 4.4.5.1
3085 | 3.18.3.1 | 4.4.5.1 | Error message in the cellular upgrade web page. →Upgrade to 4.4.5.1
3090 | 4.4.4.1 | 4.4.5.1 | If the product is configured as DHCP client, and the DHCP server doesn't send NTP server information in the lease, the NTP setting in the product is lost. →Upgrade to 4.4.5.1
3093 | 4.4.4.1 | 4.4.5.1 | For some countries, it is not possible to configure the 802.11 mode. →Upgrade to 4.4.5.1
3094 | 4.0.0.1 | 4.8.0.1 | The cloning feature (profinet or wired) doesn't work. →Upgrade to 4.8.0.1
3097 | 4.0.0.1 | 4.8.0.1 | If the Wi-Fi interface is bridged to another interface and configured to use the '4 addr format (wds)', the WPA/WPA2-EAP security policy doesn't work. The authentication is not possible. →Upgrade to 4.8.0.1
3099 | 4.0.0.1 | 4.8.0.1 | The identity parameter is required for EAP-TLS authentication. For compatibility reason, the identity 'Acksys' is used if the parameter is not set. →Upgrade to 4.8.0.1
3105 | 4.8.0.1 | 4.10.0.1 | In cluster mode "group for scanning", The scan duration for DFS channel is more important then the version 3. →Upgrade to 4.10.0.1
3123 | 4.8.0.1 | 4.8.1.1 | The USB clock is not configured correctly on the Railbox. At boot time, the cellular card can be not detected. →Upgrade to 4.8.1.1
3230 | 4.8.0.1 | 4.8.1.1 | At startup, if the cellular card is not detected, the cellular configuration is cleared. →Upgrade to 4.8.1.1
3195 | 4.10.0.1 | 3.18.3.1 | In AP mode, after a DFS event the AP is configured as isolated AP. →Upgrade to 4.10.0.1
3202 | 4.8.0.1 | 4.10.0.1 | After a reset to factory settings, the web page Status/Wireless show an error. →Upgrade to 4.10.0.1 or reboot the product
3216 | 4.8.0.1 | 4.10.0.1 | The web Page wireless/survey allow a script injection by the URL. That can allow to execute malicious code. →Upgrade to 4.10.0.1
3245 | 4.8.0.1 | 4.10.0.1 | In Alarm/event feature, the pinger event doesn't work correctly. →Upgrade to 4.10.0.1
3248 | 4.8.0.1 | 4.10.0.1 | The system cron log can be not properly applied. →Upgrade to 4.10.0.1
3308 | 4.10.0.1 | 4.14.0.1 | Typo error in the web page setup->alarms/events →Upgrade to 4.14.0.1
3232 | 3.18.0.1 | 4.10.0.1 | When a cloning mode is enabled on the wifi interface, sometimes, after cloning the signal level is not correct and the wifi client cannot associate with the AP. →Upgrade to 4.10.0.1
3235 | 4.8.0.1 | 4.14.0.1 | If the product have 2 wifi cards, the log level for wifi client mode of the second radio is not applied. →Upgrade to 4.14.0.1
3264 | 4.8.0.1 | 4.10.1.1 | It is not possible to load an AirBox V1 configuration file in the AirBox V2 product. →Upgrade to 4.10.1.1
3275 | 4.8.0.1 | 4.10.1.1 | On 11ac wifi cards, if only the antenna 1 is set, the wifi services doesn't work properly. →Upgrade to 4.10.1.1
3396 | 4.10.0.1 | 4.10.1.1 | In some cases, the products may revert to default settings after power cycling. →Impacted product: AirLink, AirBox, RuggedAir, EmbedAir, AirXroad, WaveNet-EX →Upgrade to 4.10.1.1
3398 | 4.16.9.1 | 4.18.0.1 | It is possible to configure roaming CBB with one card disabled and is not possible to enable it after CBB settings. →Upgrade to 4.18.0.1 or reset to factory settings
3406 | 4.10.0.1 | 4.12.0.1 | WEP security can be set, but this security mode is not supported by driver. →Upgrade to 4.12.0.1
3410 | 4.10.0.1 | 4.12.0.1 | The OIDs under lanInterface doesn't work correctly. →Upgrade to 4.12.0.1 or use the OIDs under networkConfiguration and networkStatus
3419 | 4.10.0.1 | 4.12.1.1 | The spectral analyzer from the WEB interface doesn't work (Site Survey). →Upgrade to 4.12.1.1
3423 | 4.8.0.1 | 4.12.1.1 | In rare cases, when wifi roaming is enabled, it may take a long time to recover the WiFi link after a communication error with the new AP. To prevent any hardware failure an optional watchdog has been added.
3430 | 3.18.3.1 | 4.14.0.1 | The status of service HTTP/HTTPS is not correct from SNMP interface →Upgrade to 4.14.0.1
3431 | 4.10.0.1 | 4.12.1.1 | If a client roam between Acksys APs, the communication can stop. →Impacted product: RuggedAir1000, Airbox
3437 | 4.12.0.1 | 4.12.1.1 | When the VRRP service is enabled, it does not notify other VRRP routers when it needs to shut down (to apply settings or to reboot the product).
3457 | 4.8.0.1 | 4.12.1.1 | If the network IP scheme in the network is not compatible with the RFC1918, some access problem to the builtin WEB server may happen.
3463 | 4.12.0.1 | 4.12.2.1 | If you define an 802.1q virtual interface with VLAN ID equal to 1, in some cases adding a new 802.1q virtual interface may change the configuration of other 802.1q virtual interfaces already present.
3475 | 4.10.0.1 | 4.12.2.1 | From the site survey, it is not possible to join an AP with WPA3 security.
3444 | 4.10.0.1 | 4.12.2.1 | The WPA3 status is not correct from SNMP. WaveManager is not able to show correctly the WPA3 settings, and in the site survey from the WEB interface, the security mode is not correct.
3472 | 4.10.0.1 | 4.12.2.1 | The VLAN priority is not correctly handled on the WiFi interfaces. All frames are sent with the BE policy regardless of the frame priority.
3476 | 4.10.0.1 | 4.12.2.1 | In the Site Survey from SNMP interface, the WPA3 security mode is not correctly handled. The security mode shown is not correct.
3549 | 4.12.1.1 | 4.14.0.1 | The wac deamon can crash when a sta attempt to make a connection with the AP. →Upgrade to 4.14.0.1
3552 | 4.12.0.1 | 4.14.0.1 | In PLH feature for rear position, in some case the selected AP is not the better →Upgrade to 4.14.0.1
3575 | 4.8.0.1 | 4.14.0.1 | In roaming situation (with roaming feature enabled) the communication can be hang for 5s. →Upgrade to 4.14.0.1
3577 | 4.10.0.1 | 4.14.0.1 | With CBB feature enabled, the communication can be hang for random duration from 1s to 5s. →Upgrade to 4.14.0.1
3581 | 4.12.2.1 | 4.14.0.1 | The bridge filter feature doesn't work correctly →Upgrade to 4.14.0.1
3597 | 4.12.0.1 | 4.14.0.1 | In rarely case, the product with an LTE interface can't boot correctly. →Upgrade to 4.14.0.1
3603 | 4.12.1.1 | 4.14.0.1 | Wac feature can't use the ssid if it contain a dot. →Upgrade to 4.14.0.1
3608 | 4.10.0.1 | 4.14.2.1 | In roaming case, the communication can be broken for several seconds. →Upgrade to 4.14.2.1
3628 | 4.12.0.1 | 4.14.2.1 | In CBB/PLH settings, some roaming doesn't work as expected. →Upgrade to 4.14.2.1
3631 | 4.12.0.1 | 4.14.1.1 | In WAC feature, the RSSI threshold is to strict. Some case the client is not able to do a connection with the AP. →Upgrade to 4.14.1.1
3632 | 4.12.0.1 | 4.14.0.1 | On 11ac wifi card, it is not possible to receive packets over 1500 bytes in length. →Upgrade to 4.14.0.1
3651 | 4.14.0.1 | 4.14.1.1 | For the product with LTE interface, the interface is disabled after upgrade to 4.14.0.1 →Upgrade to 4.14.1.1 or reload the configuration.
3681 | 4.14.0.1 | 4.14.2.1 | In CBB roaming case, some time the card switch can failed. The occurence of this issue is very rarely and occur when the roaming stress is hight. →Upgrade to 4.14.2.1
3683 | 4.14.0.1 | 4.14.1.1 | If the product is updated from WaveOS version 3.x to waveOS version 4.14.0.1, the product will return to the factory state. Don't use the version 4.14.01 to upgrade product from 3.x. →Upgrade to 4.14.1.1 or reload the configuration after upgrade.
3710 | 4.14.1.1 | 4.14.2.1 | The channel HT40 and HT80 using the channel 144 is not available. →Upgrade to 4.14.2.1
3712 | 4.14.0.1 | 4.14.2.1 | On trafic received from the ethernet interface of railbox, it is possible to have more 1‰ frame out of order. →Upgrade to 4.14.2.1
3718 | 4.14.0.1 | 4.14.2.1 | In VRRP settings case, the static route are lost when the device back to master device. →Upgrade to 4.14.2.1
3721 | 4.14.0.1 | 4.14.2.1 | In VRRP + CBB settings case, When VRRP state change, the GARP sent can be used an bad mac address. →Upgrade to 4.14.2.1
3759 | 4.14.1.1 | 4.14.2.1 | The communication between two equipment in ad-hoc wifi mode doesn't work. →Upgrade to 4.14.2.1
3761 | 4.14.1.1 | 4.14.2.1 | In case of VRRP settings, some time when the service is reloaded the backup device can get the master state. →Upgrade to 4.14.2.1
3764 | 4.14.0.1 | 4.14.2.1 | The WEP encryption doesn't work with ad-hoc wifi mode. →Upgrade to 4.14.2.1
3767 | 4.14.0.1 | 4.14.2.1 | The number of HT80 channel is not conform to the 802.11 Anexe E standard. →Upgrade to 4.14.2.1
3769 | 4.14.1.1 | 4.14.2.1 | In case of multi-ssid client settings, it is not possible to configure WPA3 encryption. →Upgrade to 4.14.2.1
3770 | 4.14.1.1 | 4.16.0.1 | the OID .1.3.6.1.4.1.28097.7.12.1.21 return the RSSI value on 40 bits. Some SNMP client/librairie are not able to decode this format. Reduce the value length to be compatible with mode SNMP client/librairy. →Upgrade to 4.16.0.1
3775 | 4.16.9.1 | 4.18.0.1 | The Wireless Access Control (WAC) is renamed to Wireless Load Balancing (WLB). →Upgrade to 4.18.0.1
3778 | 4.14.1.1 | 4.14.2.1 | The file generated by the roaming log export from the web interface don't have the correct format. →Upgrade to 4.14.2.1
3782 | 4.14.1.1 | 4.16.0.1 | Allow configuration file compatibility between AirBox/14 and AirBox/17 →Upgrade to 4.16.0.1
3811 | 4.10.0.1 | 4.16.1.1 | In some case, the Collectd demon (for telemetry feature) crash at start up. →Upgrade to 4.16.1.1
3814 | 4.16.0.1 | 4.16.1.1 | Reduce WACD memory consumption. →Upgrade to 4.16.1.1
3818 | 4.16.0.1 | 4.18.0.1 | The distance parameter is not available on the 11ac Wave2 interface, but the parameter is present in the Web interface. →Upgrade to 4.18.0.1
3819 | 4.16.0.1 | 4.18.0.1 | In the port list showed in the web interface, some row have a wrong color. The row color can change after page refresh. →Upgrade to 4.18.0.1
3821 | 4.14.1.1 | 4.16.2.1 | The Wifi led on Airxroad/4P are not correctly managed. →Upgrade to 4.16.2.1
3823 | 4.16.1.1 | 4.16.2.1 | In some cases, the roaming controle of Wireless Access Controler does not work correctly. Some sta, can be rejected from all AP. →Upgrade to 4.16.2.1
3824 | 4.16.0.1 | 4.16.2.1 | In Wireless Access Controler feature, If the roaming was globaly enabled but disabled for only one SSID, in some case the AP can disconnect a sta from this AP without reason. →Upgrade to 4.16.2.1
3827 | 4.16.0.1 | 4.16.2.1 | For SRCC feature, the configuration file generated with a WaveOS version prior than 4.16.0.1 does not work with WaveOS the versions 4.16.0.1 and 4.16.1.1 →Upgrade to 4.16.2.1
3828 | 4.16.0.1 | 4.16.2.1 | In some cases, SRCC can generate a network loop in a coach. →Upgrade to 4.16.2.1
3829 | 4.16.0.1 | 4.16.2.1 | the default ouput log level of collectd service (for telemetry feature) is DEBUG. This settings generate a lof message in the log file. →Upgrade to 4.16.2.1
3832 | 4.16.2.1 | 4.18.0.1 | The RogueAP log parameters are showed even if the feature is not enabled. →Upgrade to 4.18.0.1
3833 | 4.16.1.1 | 4.16.7.1 | In some case, the telemetry service crash. →Upgrade to 4.16.7.1
3835 | 4.16.2.1 | 4.16.3.1 | The Wac feature can disconnect the client and does not allow the client reconnexion in case of the client retry on the same AP. →Upgrade to 4.16.3.1
3836 | 4.16.2.1 | 4.16.3.1 | In some case, the wac feature compute the best AP with outdated values. →Upgrade to 4.16.3.1
3837 | 4.16.3.1 | 4.16.4.1 | If the client is connected on the AP, but doesn't transmit any packet, the signal level used by wac is not correct. →Upgrade to 4.16.4.1
3838 | 4.16.3.1 | 4.16.4.1 | In some case, the wac can use outdated information to select the best AP. This issue was introduced with the fix #3836. →Upgrade to 4.16.4.1
3839 | 4.16.4.1 | 4.16.5.1 | In the WEB UI, the password field doesn't have the focus by default. →Upgrade to 4.16.5.1
3840 | 4.16.4.1 | 4.16.5.1 | In wac feature the connected client informations are refreshed two time for each poll. →Upgrade to 4.16.5.1
3844 | 4.16.5.1 | 4.16.6.1 | In some case in wac feature, the client information has flushed when a neighbor AP refuse the association. →Upgrade to 4.16.6.1
3847 | 4.16.1.1 | 4.16.7.1 | In telemetry service, the timestamp doesn't work correctly on product range AIR* (AirLink, AirXroad, EmbedAir, AirBox,...) →Upgrade to 4.16.7.1
3853 | 4.14.0.1 | 4.18.0.1 | The discover service doesn't work correctly if we have two network with a default gateway for eeach network. The returned gateway to WaveManager is the gateway with the lowest metric. →Upgrade to 4.18.0.1
3863 | 4.14.1.1 | 4.16.9.1 | The product with 11ac Wave2 wifi board may have a wrong wifi band selected when the configuration is file is loaded. →Upgrade to 4.16.9.1
3864 | 4.14.0.1 | 4.16.9.1 | When the telemetry feature and roaming feature is enabled, in rarely case the wifi interface can be hung. →Upgrade to 4.16.9.1
3875 | 4.16.9.1 | 4.18.0.1 | The GRE configuration from the 3.x version is not correctly imported after upgrade to version 4.x. →Upgrade to 4.18.0.1
3876 | 4.16.9.1 | 4.18.0.1 | Set a STP/RSTP priority to a GRE interface is not available. →Upgrade to 4.18.0.1
3897 | 4.16.0.1 | 4.18.0.1 | The STP/RSTP status web page doesn't work. →Upgrade to 4.18.0.1
3906 | 4.14.0.1 | 4.18.5.1 | Some IPV6 frame can be sent even if the IPV6 is not configured in the product. →Upgrade to 4.18.5.1
3928 | 4.16.9.1 | 4.18.0.1 | On ruggedAir 1000 the management of wifi status LED is wrong. →Upgrade to 4.18.0.1
3950 | 4.18.0.1 | 4.18.1.1 | The wifi activity LED work only for received data →Upgrade to 4.18.1.1
3957 | 4.16.9.1 | 4.18.2.1 | If the WPA1/2/3 security is set, the communication can hang sometimes. →Upgrade to 4.18.2.1 or 4.16.12.1
3963 | 4.18.0.1 | 4.18.1.1 | If the regulation domain is set to ETSI country, it is not possible to configure the some wifi paremeters. →Upgrade to 4.18.1.1
3979 | 4.0.0.1 | 4.16.12.1 | In SRCC V1 (legacy), data packets priority is temporarily dropped during wireless transfer. They recover their priority at receipt upon decapsulation. →Upgrade to 4.16.12.1
3980 | 4.16.9.1 | 4.18.5.1 | The ntp client does not send any log. It is not possible to know when the date of product is synchronized. →Upgrade to 4.18.5.1
3983 | 4.18.0.1 | 4.18.3.1 | The pimd service doesn't start correctly on Air* products range (AirBox, Airlink, ...). Save the information on this page, and apply on another page or upgrade to 4.18.3.1
3984 | 4.18.2.1 | 4.18.1.1 | The wifi settings with multi-channel doesn't work. The product can select another channel. →Upgrade to 4.18.2.1
3985 | 4.18.2.1 | 4.18.1.1 | If the wifi channel is set to 82MHz, the wifi service doesn't start. →Upgrade to 4.18.2.1
4000 | 4.18.2.1 | 4.18.1.1 | If the product is upgraded from V3.18.x.1 to V4.18.0.1, after the upgrade, it is not possible to change the 802.11 mode. To allow the modification, the user must reset the settings to factory default. →Upgrade to 4.18.2.1
4007 | 4.18.0.1 | 4.18.3.1 | On the railbox/07, The save and apply from the page "setup → wireless interface overview" return an error. Save the information on this page, and apply on another page or upgrade to 4.18.3.1
4010 | 4.18.2.1 | 4.18.3.1 | On the railbow/07, the led management during the boot sequence is not correct. →Upgrade to 4.18.3.1
4015 | 4.18.2.1 | 4.18.3.1 | On the AirWan, the log setting page doesn't work correctly. →Upgrade to 4.18.3.1
4029 | 4.18.0.1 | 4.18.3.1 | On the Air* products ranges, it is not possible to set a password. If you upgrade a product, with a password set, with version from 4.18.0.1 to 4.18.2.1, your password will be always refused. →Upgrade to 4.18.3.1
4034 | 4.18.0.1 | 4.18.4.1 | On the Air* products ranges, the channel 144 is available in the webUI but the wireless radio radio does not support this channel. →Upgrade to 4.18.4.1
4039 | 4.16.9.1 | 4.18.7.1 | Change the log level for message "EAPOL Session ID not available". That will remove this message in the log in default loglevel. →Upgrade to 4.18.7.1
4050 | 4.18.0.1 | 4.18.4.1 | Fix for all situation the same issud of #4029 →Upgrade to 4.18.4.1
4060 | 4.16.0.1 | 4.18.5.1 | The signature of the configuration file change if the date of product is modified by the web interface. →Upgrade to 4.18.5.1
4062 | 4.22.2.1 | 4.20.0.1 | On railbox V2 with 11ax wifi card, the automatic channel and HT40- settings doesn't work.
4066 | 4.18.0.1 | 4.18.5.1 | When the mode 802.11n is set with HT40+ or HT40-, it is not possible to select the channel. →Upgrade to 4.18.5.1
4068 | 4.18.0.1 | 4.18.6.1 | When the mode 802.11n is set on 5Ghz band, the wifi service doesn't start. →Upgrade to 4.18.6.1
4069 | 4.16.9.1 | 4.18.7.1 | In some case, the AP stop to forward packet to the wifi clients. →Upgrade to 4.18.7.1
4087 | 4.20.0.1 | 4.20.1.1 | On railbox/22A0 V2, the wifi activity led does not work correctly. →Upgrade to 4.20.1.1
4098 | 4.20.0.1 | 4.20.2.1 | On RailboxV2, the wifi led activity for wifi6 interface, doesn't blink correctly. →Upgrade to 4.20.2.1
4097 | 4.20.0.1 | 4.20.2.1 | On RailboxV2, sometime the reset to factory settings doesn't work correclty →Upgrade to 4.20.2.1
4110 | 4.20.2.1 | 4.20.3.1 | On RailboxV2 with wifi6 interface, the dfs detection is not enabled →Upgrade to 4.20.3.1
4117 | 4.20.2.1 | 4.20.3.1 | On RailboxV2 with wifi6 interface, it is not possible to change the band of wifi radio →Upgrade to 4.20.3.1
4118 | 4.20.2.1 | 4.20.3.1 | On RailboxV2, the fix applied on isue #4097, does not fix the reset factory settings in all cases. →Upgrade to 4.20.3.1
4119 | 4.20.2.1 | 4.20.3.1 | On RailboxV2/DD, the password doesn't work correctly. →Upgrade to 4.20.3.1
4120 | 4.20.2.1 | 4.22.0.1 | In some case, the status cellular can show an internaly error →Upgrade to 4.22.0.1
4140 | 4.18.5.1 | 4.22.0.1 | The dns query tools doesn't work. →Upgrade to 4.22.0.1
4154 | 4.18.0.1 | 4.22.0.1 | In some cases, the telemetry service is not stable (crash or not respond). →Upgrade to 4.22.0.1
4157 | 4.18.0.1 | 4.22.0.1 | the OIDs below .1.3.6.1.4.1.28097.10.9.6 do not respond →Upgrade to 4.22.0.1
4177 | 4.20.0.4 | 4.22.0.1 | The GNSS status in deviceinfo page is not updated. →Upgrade to 4.22.0.1
4189 | 4.16.0.1 | 4.22.0.1 | If the IPV6 prefix is used to configure the IPV6 address of product, it possible to have an IPV6 conflict if several product used the same prefix. →Upgrade to 4.22.0.1
4196 | 4.16.12.1 | 4.22.3.1 | The wlb deamon have a memory leak. In some case the product will reboot if all memory are consumed. →Upgrade to 4.22.3.1
4197 | 4.22.0.1 | 4.22.1.1 | For products Railbox/DDxx V2, the feature bridgeVlan with multiple SSID doesn't work. →Upgrade to 4.22.1.1
4198 | 4.22.0.1 | 4.26.0.1 | It is not possible to set a static route without a gateway →Upgrade to 4.26.0.1
4201 | 4.18.8.1 | 4.22.2.1 | The Qatar regulation domain is not compliant with the information provided by the 3.X version. →Upgrade to 4.22.2.1
4208 | 4.24.0.1 | 4.24.4.1 | If an ipsec link is forwarded by a zone whith Ip masquerading enabled, it is not possible to communicate with IPSEC.
4214 | 4.22.0.1 | 4.22.2.1 | If the product has been updated to version 4.20.2.1 and upgraded to version 4.22.0.1, the access to the web interface is not possible (the pasword is always rejected). The same issue is present, if you load un WaveOS 4.22.0.1 the configuration from 4.20.2.1. →Upgrade to 4.22.2.1 or reset the configuration to factory values.
4220 | 4.22.0.1 | 4.22.2.1 | In some case the GNSS information is not available in WaveOS, but the GNSS is corectly fixed. →Upgrade to 4.22.2.1
4228 | 4.22.1.1 | 4.22.2.1 | SRCC data forward doesn't work on the railbox V2 products. →Upgrade to 4.22.2.1
4232 | 4.22.0.1 | 4.22.2.1 | In some case, the WaveOS upgrade on RailboxV2 will reset the configuration to the factory values →Upgrade to 4.22.2.1
4236 | 4.22.0.1 | 4.22.2.1 | In some case, The Cellular data cound doesn't work. →Upgrade to 4.22.2.1
4238 | 4.22.0.1 | 4.22.2.1 | In some case, The Cellular status show on web interface is not updated. →Upgrade to 4.22.2.1
4243 | 4.22.2.1 | 4.24.0.1 | On railbox/DVA0 V2 the manual switch sim from SNMP doesn't work.
4256 | 4.22.0.1 | 4.24.0.1 | DDNS service is not integrated in firmware image of railbox V2 WIFI4/Wifi5
4260 | 4.22.2.1 | 4.26.0.1 | The NAT 1:1 rules does not allow to configure the protocol. Only TCP and UDP worked.
4265 | 4.22.3.1 | 4.24.4.1 | If we try to change the password for the web interface (user or root), the new password is stored but an error is showed on the web interface.
4277 | 4.22.3.1 | 4.24.0.1 | The bridge filter doesn't work on wifi6 products.
4261 | 4.22.2.1 | 4.24.0.1 | SRCC in double link settings doesn't work correctly in some case.
4262 | 4.22.2.1 | 4.24.1.1 | It is not possible to disable the IPV6 network stack.
4263 | 4.22.2.1 | 4.24.0.1 | In wifi client mode, sometime the deamon crash.
4279 | 4.22.3.1 | 4.24.0.1 | Some crash occurs in AP service and WLB service when the both services are enabled
4294 | 4.22.3.1 | 4.24.0.1 | The wifi client service is not respawned when the service crash.
4305 | 4.20.0.1 | 4.24.0.1 | The wifi- product in AP mode are limited to 128 client connected.
4306 | 4.20.0.1 | 4.24.0.1 | Memory leak in WIFI6 (11ax) driver.
4315 | 4.24.0.1 | 4.24.4.1 | The channel 50 in HE160 is not allowed.
4320 | 4.22.0.1 | 4.24.0.1 | On railbox V2, after WaveOS upgrade the configuration migration doesn't work correctly.
4323 | 4.24.0.1 | 4.24.1.1 | On railbox V2 with 11ax wifi card, the bridging mode arpnat doesn't work.
4328 | 4.24.0.1 | 4.24.1.1 | The vrrp switch managed by snmp interface, stop to work after some switches.
4330 | 4.22.0.1 | 4.24.1.1 | For product with 11ac wifi card, in client mode, the wifi state is associated
4334 | 4.22.3.1 | Not fixed | On Railbox with wifi 6 card, it is not possible to change the wifi band by SNMP.
4342 | 4.22.0.1 | 4.24.1.1 | Rarely, it is not possible to upgrade the railbox V2 product.
4346 | 4.24.1.1 | 4.26.0.1 | After an reset to factory settings, waveManager may detect an IP conflic for the product. →Reboot the product or upgrade to 4.26.0.1
4357 | 4.24.0.1 | 4.24.4.1 | If a 160 MHz channel is set and the primary channel selected is not compatible with HT40+, the AP service doesn't start.
4358 | 4.24.0.1 | 4.24.4.1 | On the product wifi 6 compatible, it is not possible to disable the ht_scan on the 2.4Ghz band.
4334 | 4.22.3.1 | 4.24.5.1 | The OID to configure the 11ax radio are not present in the Acksys MIB
4362 | 4.22.3.1 | 4.24.5.1 | It is not possible to get a DHCP lease if the product is client mode with bridging mode set to arpnat.
4373 | 4.24.4.1 | 4.26.0.1 | On product with 11ac wifi interface, during the WPA rekeying the EAPOL frame are mal formed. This issue may disturb the rekeying mechanisme.
4373 | 4.26.0.1 | 4.26.1.1 | The IPSEC secret is showed in plain text.
| 4383 | 4.24.1.1 | 4.26.0.1 | On product with 11ac/11ac Wave2/11ax wifi interface, after an configuration file is loaded, the wifi mac addr used are the mac adress stored in the configuration file. The fix of this issue will increase the reboot delay juste after the configuration file is loaded. →Reboot the product or upgrade to 4.26.0.1
4389 | 4.24.2.1 | 4.26.0.1 | In roaming mono-radio condition, the wpa_supplicant deamon (to manage the wifi client side) may crash when the roaming occurs.
4424 | 4.26.0.1 | 4.26.1.1 | It is not possible to delete an wifi interface.
4442 | 4.22.2.1 | 4.28.1.1 | It is possible to add wifi interface in cellular network. This settings doesn't work
4447 | 4.28.0.1 | 4.28.1.1 | In service/statistics, it is possible to enable the cellular statistic on product without cellular interface.
4452 | 4.28.0.1 | 4.28.1.1 | no scan result is returned when a scan request is sent by mqtt
4453 | 4.28.0.1 | 4.28.1.1 | In the scan result returned by mqtt, the security field is not correct.
4454 | 4.28.0.1 | 4.28.1.1 | It is not possible to start a scan by mqtt if the radio is disabled.
4455 | 4.28.0.1 | 4.28.1.1 | If the MQTT connection is broken or a long time, the connection doesn't restart when it is possible to reach the broker.
4457 | 4.28.0.1 | 4.28.1.1 | WaveManager show a configuration waits to be applied, but no all configuration has been alredy applied.
4461 | 4.26.1.1 | 4.28.1.1 | In some cases, it is possible to lost the celullar data conexion, and it is not possible to recover it. Add product reboot to fix this case.
4463 | 4.24.0.1 | 4.28.1.1 | On railbox/DD, it is not possible to set an AP on channel 153 with HT20. In this case, the AP is up on channel 157.
4463 | 4.28.0.1 | 4.28.1.1 | On railbox/DD, it is not possible to configure an AP HE80 or HE80+80. In this case the service doesn't start.
4466 | 4.28.2.1 | 4.28.3.1 | From Mqtt interface it is not possible to change the wifi mode and the wifi band.
4474 | 4.28.1.1 | 4.28.2.1 | On railbox V2 products, it is not possible to configure the logging to be stored on the product's flash.
4492 | 4.28.2.1 | 4.28.3.1 | In a noisy environment, the loss of association frames will lead to latency in roaming performance.
4508 | 4.28.1.1 | 4.28.2.1 | On products with cellular interface, it is not possible to set a firewall zone for the cellular network.
4513 | 4.28.1.1 | 4.28.2.1 | On railbox/DS, sometimes the timeout for cellular detection may be too short.
4595 | 4.28.2.1 | 4.28.3.1 | On railbox with 11ax interface, the roaming tools doesn't work.
4607 | 4.28.3.1 | 4.28.4.1 | The RSTP parameters (path cost, port priority) are not applied to the SRCC GRE tunnel.
4644 | 4.28.3.1 | 4.28.5.1 | The RSTP parameters (path cost, port priority) are not applied to the GRE tunnel.
4646 | 4.28.3.1 | 4.28.5.1 | The RSTP parameters (path cost, port priority) are not applied to the wifi client on WDS mode.
4684 | 4.28.5.1 | 4.28.6.1 | It is not possible to connect the openvpn client to the Azur openvpn server.
4709 | 4.28.3.1 | 4.28.6.1 | It is not possible to view the GPS information in WaveManager.
4711 | 4.22.1.1 | 4.32.3.1 | With certain access points, under specific roaming conditions, IP connectivity may be lost after a roam.
4716 | 4.28.5.1 | 4.28.6.1 | On railbox V2, when the logs are saved in the product, the most recent log are not included in the archive downloaded from the web interface.
4753 | 4.28.6.1 | 4.32.3.1 | The wifi scan results is not transmited to WaveManager.
4889 | 4.28.5.1 | 4.30.0.1 | The bandwidth tools doesn't work correctly.
4748 | 4.28.3.1 | 4.32.0.1 | For 11ac products, if the device is in a noisy environment, it is sometimes connected but unable to communicate
4750 | 4.28.5.1 | 4.30.0.1 | Sometimes, the rogueAP service fails to detect access points.
4763 | 4.28.5.1 | 4.30.0.1 | It is not possible to change the active SIM from the web interface or via SNMP.
4795 | 4.28.5.1 | 4.30.0.1 | For AirboxV4 and Railbox/DV, the default number of antennas used is incorrect.
4816 | 4.28.6.1 | 4.32.0.1 | For 11ax products, if the radio is configured in client mode, it is not able to detect when the access point is lost
| 4854 | 4.28.6.1 | 4.32.1.1 | Airbox V3 does not support configuration files created with Airbox V4. | 4858 | 4.28.6.1 | 4.32.2.1 | The openVPN server doesn't work. | 4919 | 4.28.5.1 | 4.32.1.1 | The wifi client service (wpa_supplicant) can crash in roaming condition.
4923 | 4.30.0.1 | 4.32.0.1 | For 11ax product the status→wireless→status does not work.
4945 | 4.28.6.1 | 4.32.1.1 | It is not possible to create a VLAN interface on the Wi-Fi 6 interface.
4973 | 4.28.5.1 | 4.32.0.1 | Sometimes the cellular radio loses the data connection and is unable to automatically reconnect and obtain a new IP address
4995 | 4.30.0.1 | 4.32.4.1 | Static route configuration fields were not properly validated. Invalid route syntax could be entered, resulting in the route not being applied.
5000 | 4.28.6.1 | 4.32.1.1 | Intermittent SIM detection issues may occur.
5018 | 4.28.6.1 | 4.32.3.1 | In the multi-ssid configuration, the user identity field is not present.
| 5021 | 4.28.6.1 | 4.32.1.1 | Due to improper handling of the Australian regulatory domain, the Wi-Fi interface cannot be configured.
5025 | 4.30.0.1 | 4.32.0.1 | When the product upgrade starts, the countdown does not work.
| 5034 | 4.32.0.1 | 4.32.1.1 | The previous fix (bug #4816) does not totally address the case where the current AP is lost and no other AP is available. | 5039 | 4.32.0.1 | 4.32.1.1 | Railbox V2 (non-Wi-Fi 6 version) is not compatible with WaveManager 4.6 and above | 5047 | 4.30.0.1 | 4.32.2.1 | in wifi configuration page, it is not possible to upload the certificat required by WPA/2/3-ENTERPRISE. | 5048 | 4.28.6.1 | 4.32.2.1 | The ping failure event doesn't allow to shutdown the wifi interface in all cases. | 5049 | 4.32.0.1 | 4.32.1.1 | SNMPv1 is disabled in the web UI, but the service is still active and accessible externally. | 5051 | 4.32.0.1 | 4.32.4.1 | The firewall does not drop execisive http connexion | 5052 | 4.32.0.1 | 4.32.4.1 | The firewall does not drop execisive https connexion | 5073 | 4.32.1.1 | 4.32.4.1 | Creating an SNMPv3 user required running the creation process twice to take effect. | 5075 | 4.28.2.1 | 4.32.3.1 | On products equipped with a 5G modem, connecting to the cellular network may be difficult. | 5091 | 4.28.6.1 | 4.34.0.1 | On the wifi 6 channel, it is not possible to forward the frames with VLAN tags. | 5099 | 4.30.0.1 | 4.32.2.1 | It is not possible to validate an WPA/2/3-ENTERPRISE settings. | 5113 | 4.10.0.1 | 4.32.2.1 | It is impossible to configure a PSK key via SNMP if it contains a % character. | 5117 | 4.32.1.1 | 4.32.4.1 | Attachment status issue in the web interface on a 5G SA network. | 5118 | 4.32.1.1 | 4.32.4.1 | Reading the temperature via SNMP causes the service to hang. | 5126 | 4.30.0.1 | 4.32.2.1 | TLS 1.2 has been disabled for security reasons. However, many infrastructures still use this version of TLS. Added a fallback to TLS 1.2 if authentication with TLS 1.3 fails. | 5129 | 4.32.1.1 | 4.32.4.1 | The "Exclude DFS channels" setting is visible on the 2.4 GHz band.
5142 | 4.24.0.1 | 4.33.3.1 | The cellular LED continues to indicate that the modem is active even after it has been disabled.
5145 | 4.24.0.1 | 4.32.0.1 | The graphical interface for configuring the OpenVPN service does not allow the certificate to be uploaded.
| 5168 | 4.32.1.1 | 4.30.0.1 | It is not possible to define a port range longer than 5 characters in the firewall. | 5173 | 4.32.2.1 | 4.32.4.1 | On the railbox range, it is not possible to change the root password from the web interface. | 5213 | 4.32.3.1 | 4.34.0.1 | On the 6 GHz band, Preferred scanning channels do not appear in the web interface. ⇒ Allow manuel settings for this version | 5232 | 4.32.2.1 | 4.36.0.1 | The round-trip time reported by the ping command may occasionally be significantly high. | 5233 | 4.32.3.1 | 4.34.0.1 | On the 6 GHz band, it is not possible to save the Wi-Fi configuration. ⇒Workaround: In the Wireless Security tab, a PSK must be set. | 5234 | 4.32.3.1 | 4.34.0.1 | When the Saudi Arabia regulatory domain is set, it is not possible to configure the channels from the web interface on the Wi-Fi 6E radio. | 5235 | 4.32.3.1 | 4.34.0.1 | When the Australia regulatory domain is set, some ath11k error messages appear in the kernel log on the Wi-Fi 6E radio. | 5236 | 4.32.3.1 | 4.34.0.1 | Some Wi-Fi roles not supported by the hardware are shown on the 6 GHz Wi-Fi band. | 5257 | 4.32.3.1 | 4.36.0.1 | Firewall randomly block Traffic | 5260 | 4.34.0.1 | 4.36.0.1 | The DDNS status remains "Enabled" even after being disabled via SNMP | 5278 | 4.28.6.1 | 4.34.0.1 | Fixed a use-after-free issue in the PIM service. | 5293 | 4.32.6.1 | 4.36.0.1 | On 5G cellular products, static routes are not associated with the correct interface, resulting in traffic not being forwarded.

back to top

Changes Log Known issues
WaveOS changes log, 17-June-2026
Software and documentation copyright by Acksys, 2026 - all rights reserved